(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 187)
    (zones 0)
    (modules 19)
    (nets 14)
  )

  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 +15V)
  (net 2 GNDA)
  (net 3 -15V)
  (net 4 "Net-(RA3-Pad2)")
  (net 5 "Net-(RB3-Pad2)")
  (net 6 in_outA)
  (net 7 out_inA)
  (net 8 in_outB)
  (net 9 inA+)
  (net 10 out_inB)
  (net 11 inB+)
  (net 12 "Net-(JA1-Pad2)")
  (net 13 "Net-(JB1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(JA1-Pad2)")
    (add_net "Net-(JB1-Pad2)")
    (add_net "Net-(RA3-Pad2)")
    (add_net "Net-(RB3-Pad2)")
    (add_net inA+)
    (add_net inB+)
    (add_net in_outA)
    (add_net in_outB)
    (add_net out_inA)
    (add_net out_inB)
  )

  (net_class power ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net -15V)
    (add_net GNDA)
  )

  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5) (tstamp 5C548E98)
    (at 101.6 40.64)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (path /5C54CA7D)
    (fp_text reference U1 (at 3.81 1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM4562 (at 3.81 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 8.89) (end 0.635 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 8.95) (end 6.46 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 8.95) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.1 -1.55) (end -1.1 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.1 9.15) (end 8.7 9.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 9.15) (end 8.7 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 in_outA))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 out_inA))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(RA3-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 in_outB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C549AAD)
    (at 96.52 55.88 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA8C)
    (fp_text reference RA2 (at -2.54 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 out_inA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C5492E5)
    (at 91.44 45.72)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAA4)
    (fp_text reference RA3 (at 3.81 -1.905) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(RA3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 inA+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA2AC0F)
    (at 93.98 48.26 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAB9)
    (fp_text reference RA4 (at 10.16 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10 (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(JA1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548D58)
    (at 99.06 48.26 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAAC)
    (fp_text reference RA5 (at 10.16 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(RA3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C5481CB)
    (at 119.38 43.18 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CB19)
    (fp_text reference RB1 (at 3.81 -1.905 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 in_outB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548E51)
    (at 114.3 58.42 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAD8)
    (fp_text reference RB2 (at 2.54 -1.92 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548E0F)
    (at 119.38 48.26 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAE4)
    (fp_text reference RB3 (at 3.81 1.905 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(RB3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 inB+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548D9A)
    (at 116.84 50.8 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAF8)
    (fp_text reference RB4 (at 3.81 -1.92 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10 (at 3.81 1.92 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 270) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(JB1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C548D16)
    (at 111.76 53.34 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CAEC)
    (fp_text reference RB5 (at 3.81 -1.92 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(RB3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5C549444)
    (at 91.44 40.64)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5C54CA95)
    (fp_text reference RA1 (at 10.16 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10k (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 out_inA))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 in_outA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2366A)
    (at 98.98 34.29 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (path /5CA42A5F)
    (fp_text reference ClpA1 (at -3.255 1.27 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330p (at 2.5 3 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 -1.75) (end -1 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.75) (end 6 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 1.75) (end 6 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 -1.75) (end -1 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.12 -1.87) (end 6.12 -1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end -1.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.12 -1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 -2) (end -1.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 in_outA))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 out_inA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2367D)
    (at 111.76 36.83)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (path /5CA46ED4)
    (fp_text reference ClpB1 (at 3.175 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330p (at 2.5 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.25 -2) (end -1.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.12 -1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end -1.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 1.87) (end 6.12 1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.12 -1.87) (end 6.12 -1.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 6 -1.75) (end -1 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start 6 1.75) (end 6 -1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 1.75) (end 6 1.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.75) (end -1 1.75) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 out_inB))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 in_outB))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA236AB)
    (at 99.06 38.1 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CA39C35)
    (fp_text reference RA7 (at 3.81 -4.445 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 3.81 1.92 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 180) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 in_outA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2B254)
    (at 109.22 38.1 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB2B)
    (fp_text reference C1 (at 1.25 -2.05 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CA2B18E)
    (at 104.14 50.8 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (path /5C54CB3A)
    (fp_text reference C2 (at 1.25 -2.05 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100n (at 1.25 2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 1.25 0 180) (layer F.Fab)
      (effects (font (size 0.6 0.6) (thickness 0.09)))
    )
    (fp_line (start 3.55 -1.05) (end -1.05 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 1.05) (end 3.55 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.05) (end 3.55 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 -1.05) (end -1.05 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.621 0.92) (end 1.879 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.621 -0.92) (end 1.879 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.75 -0.8) (end -0.25 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.75 0.8) (end 2.75 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 0.8) (end 2.75 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.25 -0.8) (end -0.25 0.8) (layer F.Fab) (width 0.1))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 -15V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B) (tstamp 5CA2B122)
    (at 111.76 40.64)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (path /5CA3D551)
    (fp_text reference RB6 (at 3.81 -1.92) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 220 (at 3.81 1.92) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.01 -0.8) (end 2.01 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.01 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 5.61 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.92) (end 5.73 0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.94 0) (end 1.89 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.68 0) (end 5.73 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.95 1.05) (end 8.57 1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 0.72 0.72) (thickness 0.108)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 in_outB))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66) (tstamp 5CA2B5D2)
    (at 92.06 43.18)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CACC)
    (attr virtual)
    (fp_text reference JA1 (at 3.19 0) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 3.19 -1.905) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 12 "Net-(JA1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 9 inA+) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66) (tstamp 5CA2B950)
    (at 118.745 45.72 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (path /5C54CB0B)
    (attr virtual)
    (fp_text reference JB1 (at 3.175 0 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Jumper (at 2.54 1.905 180) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start 0.7 0.3) (end 1.4 0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start 0.7 -0.3) (end 0.7 -1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 -0.3) (end -1.4 -0.3) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_arc (start -0.7 0.3) (end -0.7 1) (angle 90) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.4 -0.3) (end -1.4 0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.7 -1) (end -0.7 -1) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.4 0.3) (end 1.4 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 1) (end 0.7 1) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.65 1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.65 1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end 1.65 1.25) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.65 -1.25) (end -1.65 -1.25) (layer B.CrtYd) (width 0.05))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 11 inB+) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 13 "Net-(JB1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )

  (segment (start 109.22 38.14) (end 109.26 38.1) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 109.22 40.64) (end 109.22 38.14) (width 1) (layer B.Cu) (net 1) (status 30))
  (segment (start 102.52 66.54) (end 102.52 62.58) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.52 62.58) (end 102.87 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 104.52 62.61) (end 104.52 66.54) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 104.14 62.23) (end 104.52 62.61) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.505 62.23) (end 104.14 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 102.87 62.23) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer B.Cu) (net 1))
  (segment (start 103.52 62.245) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 103.52 66.54) (end 103.52 62.245) (width 0.5) (layer F.Cu) (net 1))
  (via (at 103.505 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 106.045 53.975) (end 103.505 56.515) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 106.045 43.815) (end 106.045 53.975) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 109.22 40.64) (end 106.045 43.815) (width 0.5) (layer F.Cu) (net 1) (status 10))
  (segment (start 103.505 56.515) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 102.87 62.23) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 102.52 62.58) (end 102.87 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 102.52 66.54) (end 102.52 62.58) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 104.52 62.61) (end 104.14 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 104.14 62.23) (end 103.505 62.23) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 104.52 66.54) (end 104.52 62.61) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 106.76 38.1) (end 105.49 39.37) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 105.49 49.41) (end 104.1 50.8) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 105.49 39.37) (end 105.49 49.41) (width 1) (layer B.Cu) (net 2))
  (segment (start 104.1 50.8) (end 104.1 54.65) (width 1) (layer B.Cu) (net 2) (status 10))
  (segment (start 104.1 54.65) (end 102.87 55.88) (width 1) (layer B.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 62.405) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 101.52 62.785) (end 101.52 66.54) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.965 62.23) (end 101.52 62.785) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 62.675) (end 100.965 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.675) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.695 62.23) (end 100.33 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.33 62.23) (end 100.965 62.23) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.52 63.04) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.52 66.54) (end 99.52 63.04) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.52 62.42) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 100.52 66.54) (end 100.52 62.42) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.52 63.42) (end 100.33 62.23) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 101.52 66.54) (end 101.52 63.42) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 99.52 62.405) (end 99.695 62.23) (width 0.5) (layer B.Cu) (net 2))
  (via (at 100.33 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 100.33 55.88) (end 99.06 55.88) (width 1) (layer B.Cu) (net 2) (status 20))
  (segment (start 102.87 55.88) (end 100.33 55.88) (width 1) (layer B.Cu) (net 2))
  (segment (start 93.98 55.88) (end 93.98 54.61) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 95.25 53.34) (end 97.79 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 93.98 54.61) (end 95.25 53.34) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 99.06 54.61) (end 99.06 55.88) (width 0.5) (layer B.Cu) (net 2) (status 20))
  (segment (start 97.79 53.34) (end 99.06 54.61) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 116.84 58.42) (end 116.84 57.15) (width 0.5) (layer B.Cu) (net 2) (status 10))
  (segment (start 116.84 57.15) (end 115.57 55.88) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 100.33 62.23) (end 100.33 53.34) (width 0.5) (layer F.Cu) (net 2))
  (via (at 100.33 55.88) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 115.489999 57.069999) (end 116.140001 57.720001) (width 0.5) (layer F.Cu) (net 2) (status 20))
  (segment (start 113.651999 57.069999) (end 115.489999 57.069999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 116.140001 57.720001) (end 116.84 58.42) (width 0.5) (layer F.Cu) (net 2) (status 30))
  (segment (start 112.52 58.201998) (end 113.651999 57.069999) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 112.52 66.54) (end 112.52 58.201998) (width 0.5) (layer F.Cu) (net 2))
  (via (at 107.95 55.88) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 115.57 55.88) (end 107.95 55.88) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 107.95 55.88) (end 102.87 55.88) (width 0.5) (layer B.Cu) (net 2))
  (segment (start 98.52 66.54) (end 98.52 62.325) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 98.52 62.325) (end 98.425 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 62.23) (end 96.52 66.04) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 97.52 62.595) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 97.52 66.54) (end 97.52 62.595) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 98.425 62.23) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 96.52 66.54) (end 96.52 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 98.52 62.325) (end 98.52 66.54) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 98.425 62.23) (end 98.52 62.325) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.52 62.595) (end 97.52 66.54) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.155 62.23) (end 97.52 62.595) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 62.23) (end 97.155 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 96.52 62.23) (end 97.79 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 97.79 62.23) (end 98.425 62.23) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 101.6 48.26) (end 101.6 50.8) (width 1) (layer B.Cu) (net 3) (status 30))
  (segment (start 97.155 57.785) (end 97.79 58.42) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 101.6 50.8) (end 95.25 50.8) (width 0.5) (layer F.Cu) (net 3) (status 10))
  (segment (start 92.075 56.515) (end 93.345 57.785) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 95.25 50.8) (end 92.075 53.975) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 93.345 57.785) (end 97.155 57.785) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 92.075 53.975) (end 92.075 56.515) (width 0.5) (layer F.Cu) (net 3))
  (segment (start 96.52 62.23) (end 97.155 62.23) (width 0.5) (layer B.Cu) (net 3))
  (segment (start 97.79 58.42) (end 97.79 62.23) (width 0.5) (layer F.Cu) (net 3))
  (via (at 97.79 62.23) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 3))
  (segment (start 118.11 45.72) (end 116.84 46.99) (width 1) (layer B.Cu) (net 13))
  (segment (start 116.84 46.99) (end 116.84 50.8) (width 1) (layer B.Cu) (net 13) (status 20))
  (segment (start 93.98 48.26) (end 93.98 44.45) (width 1) (layer B.Cu) (net 12) (status 10))
  (segment (start 119.41 48.23) (end 119.38 48.26) (width 1) (layer F.Cu) (net 11) (status 30))
  (segment (start 119.41 48.23) (end 119.38 48.26) (width 1) (layer B.Cu) (net 11) (status 30))
  (segment (start 119.41 45.72) (end 119.41 48.23) (width 1) (layer B.Cu) (net 11) (status 20))
  (segment (start 91.41 45.69) (end 91.44 45.72) (width 1) (layer B.Cu) (net 9) (status 30))
  (segment (start 99.06 43.18) (end 96.52 43.18) (width 1) (layer B.Cu) (net 7))
  (segment (start 96.52 43.18) (end 93.98 40.64) (width 1) (layer B.Cu) (net 7))
  (segment (start 93.98 40.64) (end 91.44 40.64) (width 1) (layer B.Cu) (net 7) (status 20))
  (segment (start 101.6 43.18) (end 99.06 43.18) (width 1) (layer B.Cu) (net 7) (status 10))
  (segment (start 96.52 48.26) (end 96.52 43.18) (width 1) (layer B.Cu) (net 7) (status 10))
  (segment (start 99.06 40.64) (end 101.6 40.64) (width 1) (layer B.Cu) (net 6) (status 30))
  (segment (start 101.6 45.72) (end 99.06 45.72) (width 1) (layer B.Cu) (net 4) (status 30))
  (segment (start 99.06 45.72) (end 99.06 48.26) (width 1) (layer B.Cu) (net 4) (status 30))
  (segment (start 109.22 45.72) (end 111.76 45.72) (width 1) (layer B.Cu) (net 10) (status 10))
  (segment (start 119.38 43.18) (end 116.84 43.18) (width 1) (layer B.Cu) (net 10) (status 10))
  (segment (start 114.3 45.72) (end 111.76 45.72) (width 1) (layer B.Cu) (net 10))
  (segment (start 116.84 43.18) (end 114.3 45.72) (width 1) (layer B.Cu) (net 10))
  (segment (start 114.3 50.8) (end 114.3 45.72) (width 1) (layer B.Cu) (net 10) (status 10))
  (segment (start 111.76 43.18) (end 109.22 43.18) (width 1) (layer B.Cu) (net 8) (status 30))
  (segment (start 111.76 48.26) (end 109.22 48.26) (width 1) (layer B.Cu) (net 5) (status 30))
  (segment (start 111.76 48.26) (end 111.76 53.34) (width 1) (layer B.Cu) (net 5) (status 30))
  (segment (start 98.98 38.02) (end 99.06 38.1) (width 0.5) (layer B.Cu) (net 6) (status 30))
  (segment (start 98.98 34.29) (end 98.98 38.02) (width 0.5) (layer B.Cu) (net 6) (status 30))
  (segment (start 99.06 38.1) (end 99.06 40.64) (width 0.5) (layer B.Cu) (net 6) (status 30))
  (segment (start 107.315 40.64) (end 101.6 40.64) (width 0.5) (layer F.Cu) (net 6) (status 20))
  (segment (start 107.315 45.085) (end 107.315 40.64) (width 0.5) (layer B.Cu) (net 6))
  (via (at 107.315 45.085) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (via (at 107.315 40.64) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 107.315 51.435) (end 107.315 45.085) (width 0.5) (layer F.Cu) (net 6))
  (segment (start 111.52 55.64) (end 107.315 51.435) (width 0.5) (layer F.Cu) (net 6))
  (segment (start 111.52 66.54) (end 111.52 55.64) (width 0.5) (layer F.Cu) (net 6))
  (segment (start 93.98 34.29) (end 93.98 40.64) (width 0.5) (layer B.Cu) (net 7) (status 10))
  (segment (start 92.629999 54.687195) (end 96.52 50.797194) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 96.52 50.797194) (end 96.52 48.26) (width 0.5) (layer B.Cu) (net 7) (status 20))
  (segment (start 92.629999 56.528001) (end 92.629999 54.687195) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 94.787007 58.685009) (end 92.629999 56.528001) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 111.52 60.72) (end 109.48501 58.68501) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 109.48501 58.68501) (end 94.787007 58.685009) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 111.52 60.72) (end 111.52 66.54) (width 0.5) (layer B.Cu) (net 7))
  (segment (start 116.84 38.04137) (end 116.84 43.18) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 116.76 37.96137) (end 116.84 38.04137) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 116.76 36.83) (end 116.76 37.96137) (width 0.5) (layer B.Cu) (net 10) (status 10))
  (segment (start 111.76 36.83) (end 111.76 40.64) (width 0.5) (layer B.Cu) (net 8) (status 30))
  (segment (start 111.76 40.64) (end 111.76 43.18) (width 0.5) (layer B.Cu) (net 8) (status 30))
  (segment (start 113.03 39.37) (end 111.76 40.64) (width 0.5) (layer F.Cu) (net 8) (status 20))
  (segment (start 121.63001 40.35001) (end 120.65 39.37) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 120.65 39.37) (end 120.108002 39.37) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 121.63001 56.902796) (end 121.63001 40.35001) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 119.812002 39.37) (end 120.108002 39.37) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 120.108002 39.37) (end 113.03 39.37) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 114.52 63.74) (end 114.52 66.04) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 121.63001 56.902796) (end 116.302806 62.23) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 116.302806 62.23) (end 115.57 62.23) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 114.52 63.28) (end 114.52 66.04) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 115.57 62.23) (end 114.52 63.28) (width 0.5) (layer F.Cu) (net 8))
  (segment (start 91.44 45.72) (end 91.44 56.610806) (width 0.5) (layer B.Cu) (net 9) (status 10))
  (segment (start 91.44 56.610806) (end 94.519194 59.69) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 94.519194 59.69) (end 108.585 59.69) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 110.52 61.625) (end 110.52 66.54) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 108.585 59.69) (end 110.52 61.625) (width 0.5) (layer B.Cu) (net 9))
  (segment (start 96.52 55.88) (end 96.52 56.869949) (width 0.5) (layer B.Cu) (net 0) (status 10))
  (segment (start 96.52 56.869949) (end 97.435051 57.785) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 97.435051 57.785) (end 110.49 57.785) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 110.49 57.785) (end 112.52 59.815) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 112.52 59.815) (end 112.52 66.54) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 113.52 66.54) (end 113.52 63.74) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 113.52 61.900002) (end 113.52 66.54) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 115.650001 59.770001) (end 113.52 61.900002) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 119.38 40.64) (end 120.730001 41.990001) (width 0.5) (layer F.Cu) (net 0) (status 10))
  (segment (start 120.730001 41.990001) (end 120.730001 56.529999) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 120.728003 56.529999) (end 120.730001 56.529999) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 117.488001 59.770001) (end 120.728003 56.529999) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 115.650001 59.770001) (end 117.488001 59.770001) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 110.52 66.54) (end 110.52 63.74) (width 0.5) (layer F.Cu) (net 0))
  (via (at 107.95 60.96) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 0))
  (segment (start 90.089999 56.533611) (end 90.089999 39.450001) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 90.740001 38.799999) (end 91.44 38.1) (width 0.5) (layer B.Cu) (net 0) (status 30))
  (segment (start 94.516388 60.96) (end 90.089999 56.533611) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 90.089999 39.450001) (end 90.740001 38.799999) (width 0.5) (layer B.Cu) (net 0) (status 20))
  (segment (start 107.95 60.96) (end 94.516388 60.96) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 110.495001 63.715001) (end 110.52 63.74) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 110.495001 63.505001) (end 110.495001 63.715001) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 107.95 60.96) (end 110.495001 63.505001) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 114.3 53.337194) (end 114.3 50.8) (width 0.5) (layer B.Cu) (net 10) (status 20))
  (segment (start 118.190001 59.068001) (end 118.190001 57.227195) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 118.190001 57.227195) (end 114.3 53.337194) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 114.52 60.74) (end 114.52 63.74) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 115.489999 59.770001) (end 114.52 60.74) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 114.52 63.74) (end 114.52 66.54) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 117.488001 59.770001) (end 115.489999 59.770001) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 118.190001 59.068001) (end 117.488001 59.770001) (width 0.5) (layer B.Cu) (net 10))
  (segment (start 115.52 63.010808) (end 115.52 66.54) (width 0.5) (layer B.Cu) (net 11))
  (segment (start 119.38 59.150808) (end 115.52 63.010808) (width 0.5) (layer B.Cu) (net 11))
  (segment (start 119.38 48.26) (end 119.38 59.150808) (width 0.5) (layer B.Cu) (net 11) (status 10))
  (segment (start 113.52 59.2) (end 114.3 58.42) (width 0.5) (layer B.Cu) (net 0) (status 20))
  (segment (start 113.52 60.47) (end 113.52 66.54) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 113.52 59.2) (end 113.52 60.47) (width 0.5) (layer B.Cu) (net 0))
  (segment (start 91.41 43.18) (end 91.41 45.69) (width 1) (layer B.Cu) (net 9) (status 30))
  (segment (start 92.71 43.18) (end 93.98 44.45) (width 1) (layer B.Cu) (net 12) (status 10))

  (zone (net 2) (net_name GNDA) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 32.385) (xy 123.19 32.385) (xy 123.19 64.77) (xy 88.9 64.77)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.9 32.385) (xy 123.19 32.385) (xy 123.19 64.77) (xy 88.9 64.77)
      )
    )
  )
  (zone (net 3) (net_name -15V) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.52 62.23) (xy 98.425 62.23) (xy 98.425 64.77) (xy 96.52 64.77)
      )
    )
  )
  (zone (net 1) (net_name +15V) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.87 62.23) (xy 104.14 62.23) (xy 104.775 64.135) (xy 102.235 64.135)
      )
    )
  )
  (zone (net 1) (net_name +15V) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.87 62.23) (xy 104.14 62.23) (xy 104.775 64.135) (xy 102.235 64.135)
      )
    )
  )
  (zone (net 3) (net_name -15V) (layer B.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.52 62.23) (xy 98.425 62.23) (xy 98.425 64.135) (xy 96.52 64.135)
      )
    )
  )
)
