(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)

  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 38)
    (zones 0)
    (modules 10)
    (nets 8)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 1)
    (trace_clearance 1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(C25-Pad1)")
  (net 2 "Net-(C25-Pad2)")
  (net 3 "Net-(D5-Pad1)")
  (net 4 "Net-(D5-Pad2)")
  (net 5 "Net-(F1-Pad2)")
  (net 6 "Net-(F1-Pad1)")
  (net 7 "Net-(J1-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 1)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad2)")
  )

  (module Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P10.00mm (layer F.Cu) (tedit 5AE50EF0) (tstamp 5CEFA5DA)
    (at 53.34 35.56 90)
    (descr "C, Disc series, Radial, pin pitch=10.00mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 10.00mm  diameter 14.5mm width 5.0mm Capacitor")
    (path /5BCEF457)
    (fp_text reference C25 (at 5 -3.75 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "203M SF 250V AC" (at 5 3.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.25 -2.5) (end -2.25 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.25 2.5) (end 12.25 2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 12.25 2.5) (end 12.25 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start 12.25 -2.5) (end -2.25 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.37 -2.62) (end 12.37 -2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.37 2.62) (end 12.37 2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.37 -2.62) (end -2.37 2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.37 -2.62) (end 12.37 2.62) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -2.75) (end -2.5 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.5 2.75) (end 12.5 2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.5 2.75) (end 12.5 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.5 -2.75) (end -2.5 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 10 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P10.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module mixersupply_fuse:Fuseholder0520 (layer F.Cu) (tedit 5BC4A14C) (tstamp 5CEFA605)
    (at 38.1 48.26)
    (path /5BA8F401)
    (fp_text reference F1 (at 0 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Fuse 1.6A T" (at 0 -6.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 13.97 -3.81) (end 13.97 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 13.97 3.81) (end -13.97 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -13.97 3.81) (end -13.97 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -13.97 -3.81) (end 13.97 -3.81) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad1)"))
    (pad 1 thru_hole oval (at -10.16 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad1)"))
  )

  (module mixersupply_connectors:AC_Connector (layer F.Cu) (tedit 5BC49EDC) (tstamp 5CEFA614)
    (at 20.32 30.48 90)
    (path /5BAE5D12)
    (fp_text reference J1 (at 0 -6.985 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "230V In" (at 0 -8.255 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -10.16 -3.5) (end 10.16 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 -3.5) (end 10.16 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10.16 3.5) (end -10.16 3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start -10.16 3.5) (end -10.16 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -3.556) (end 1.524 -3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 -3.556) (end 1.524 3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.524 3.556) (end -1.524 3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.524 3.556) (end -1.524 -3.556) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.524 -3.556) (end 0 -3.556) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -5.08 0 90) (size 6 6) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 6 6) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
  )

  (module mixersupply_connectors:2Pin_8mm_w_clipconnector (layer F.Cu) (tedit 5BC4A364) (tstamp 5CEFA622)
    (at 62.42 48.26 180)
    (path /5BD2B533)
    (fp_text reference J2 (at 0 -6.35 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "PWR Switch" (at 0 -7.62 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 6.35 -3.81) (end 6.35 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.35 3.81) (end -6.35 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 3.81) (end -6.35 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 -3.81) (end -5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -3.81) (end -5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -5.08) (end 5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -5.08) (end 5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -3.81) (end 6.35 -3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole oval (at 4 0 270) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 2 thru_hole oval (at -4 0 270) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 5CEFA638)
    (at 93.98 30.48 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /5CF08DB4)
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Relais_on (at 0 4.87 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module mixersupply_connectors:2Pin_8mm_w_clipconnector (layer F.Cu) (tedit 5BC4A364) (tstamp 5CEFA646)
    (at 40.64 25.4)
    (path /5BC67AD5)
    (fp_text reference J6 (at 0 -6.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Transformator Primary" (at 0 -7.62) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.08 -3.81) (end 6.35 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.08 -5.08) (end 5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -5.08) (end 5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.08 -3.81) (end -5.08 -5.08) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 -3.81) (end -5.08 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -6.35 3.81) (end -6.35 -3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.35 3.81) (end -6.35 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 6.35 -3.81) (end 6.35 3.81) (layer F.SilkS) (width 0.15))
    (pad 2 thru_hole oval (at -4 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 thru_hole oval (at 4 0 90) (size 4.5 3.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
  )

  (module "mixersupply_relay:Relais DEG SDT-S-105LMR" (layer F.Cu) (tedit 5BC4BB47) (tstamp 5CEFA652)
    (at 83.82 25.4 270)
    (path /5BD04C3D)
    (fp_text reference K1 (at 0 -10.16 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "DEG SDT-S-105LMR" (at 0 -11.43 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.81 -2.54) (end 24.13 -2.54) (layer F.SilkS) (width 0.15))
    (fp_line (start 24.13 -2.54) (end 24.13 10.16) (layer F.SilkS) (width 0.15))
    (fp_line (start 24.13 10.16) (end -3.81 10.16) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.81 10.16) (end -3.81 -2.54) (layer F.SilkS) (width 0.15))
    (pad A1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D5-Pad1)"))
    (pad A2 thru_hole circle (at 0 7.62 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D5-Pad2)"))
    (pad 11 thru_hole circle (at 16.51 7.62 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
    (pad 14 thru_hole circle (at 20.32 0 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
  )

  (module Varistor:RV_Disc_D7mm_W3.4mm_P5mm (layer F.Cu) (tedit 5A0F68DF) (tstamp 5CEFB0E9)
    (at 43.18 35.56 180)
    (descr "Varistor, diameter 7mm, width 3.4mm, pitch 5mm")
    (tags "varistor SIOV")
    (path /5BDC383D)
    (fp_text reference RV1 (at 2.5 3.35 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Varistor (at 2.5 -2.05 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 2.5 0.65 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.25 2.6) (end 6.25 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.3) (end 6.25 -1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.25 -1.3) (end 6.25 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.25 -1.3) (end -1.25 2.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 2.35) (end 6 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.05) (end 6 -1.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 -1.05) (end 6 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 -1.05) (end -1 2.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1 2.35) (end 6 2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.05) (end 6 -1.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6 -1.05) (end 6 2.35) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -1.05) (end -1 2.35) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 5 1.3 180) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D7mm_W3.4mm_P5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Varistor:RV_Disc_D21.5mm_W4.8mm_P10mm (layer F.Cu) (tedit 5A0F68FE) (tstamp 5CEFA678)
    (at 59.01 35.4 90)
    (descr "Varistor, diameter 21.5mm, width 4.8mm, pitch 10mm")
    (tags "varistor SIOV")
    (path /5BCBFCA3)
    (fp_text reference TH1 (at 5 4.375 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Thermistor_NTC (at 5 -2.425 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5 0.975 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -6 3.63) (end 16 3.63) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6 -1.68) (end 16 -1.68) (layer F.CrtYd) (width 0.05))
    (fp_line (start 16 -1.68) (end 16 3.63) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6 -1.68) (end -6 3.63) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.75 3.375) (end 15.75 3.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.75 -1.425) (end 15.75 -1.425) (layer F.SilkS) (width 0.15))
    (fp_line (start 15.75 -1.425) (end 15.75 3.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.75 -1.425) (end -5.75 3.375) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.75 3.375) (end 15.75 3.375) (layer F.Fab) (width 0.1))
    (fp_line (start -5.75 -1.425) (end 15.75 -1.425) (layer F.Fab) (width 0.1))
    (fp_line (start 15.75 -1.425) (end 15.75 3.375) (layer F.Fab) (width 0.1))
    (fp_line (start -5.75 -1.425) (end -5.75 3.375) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 10 1.95 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C25-Pad2)"))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D21.5mm_W4.8mm_P10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diode_THT:D_DO-15_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5) (tstamp 5CEFB622)
    (at 88.9 30.48 90)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 2.54mm  length 7.6mm diameter 3.6mm")
    (path /5BA90880)
    (fp_text reference D5 (at 1.27 -2.92 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value DIODE (at 1.27 3.809 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 0 0) (end 1.514596 -1.12) (angle -284.154462) (layer F.SilkS) (width 0.12))
    (fp_circle (center 0 0) (end 1.8 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.05 -2.05) (end -2.05 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.05 2.05) (end 3.91 2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.91 2.05) (end 3.91 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.91 -2.05) (end -2.05 -2.05) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.27 -2.92 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user A (at 4.66 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user A (at 4.66 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 39.37 43.18) (end 36.83 43.18) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 39.37 53.34) (end 39.37 43.18) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.83 53.34) (end 39.37 53.34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36.83 43.18) (end 36.83 53.34) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 15.24 31.75) (end 15.24 29.21) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 25.4 31.75) (end 15.24 31.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 25.4 29.21) (end 25.4 31.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 15.24 29.21) (end 25.4 29.21) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 10.16 55.88) (end 10.16 10.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.52 55.88) (end 10.16 55.88) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.52 10.16) (end 96.52 55.88) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 10.16 10.16) (end 96.52 10.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 35.56) (end 71.12 38.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.9 35.56) (end 71.12 35.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.9 38.1) (end 88.9 35.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 38.1) (end 88.9 38.1) (layer Edge.Cuts) (width 0.1))

  (via (at 15.24 15.24) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0))
  (via (at 15.24 50.8) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5CEFB3E8))
  (via (at 91.44 15.24) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5CEFB6A1))
  (via (at 91.44 50.8) (size 5) (drill 3) (layers F.Cu B.Cu) (net 0) (tstamp 5CEFB6A3))
  (segment (start 53.34 35.56) (end 43.18 35.56) (width 2) (layer B.Cu) (net 1) (status 30))
  (segment (start 81.28 48.26) (end 83.82 45.72) (width 2) (layer B.Cu) (net 1) (status 20))
  (segment (start 59.01 35.4) (end 59.01 40.35) (width 2) (layer B.Cu) (net 1) (status 10))
  (segment (start 53.5 35.4) (end 53.34 35.56) (width 2) (layer B.Cu) (net 1) (status 30))
  (segment (start 59.01 35.4) (end 53.5 35.4) (width 2) (layer B.Cu) (net 1) (status 30))
  (segment (start 66.42 48.26) (end 81.28 48.26) (width 2) (layer B.Cu) (net 1))
  (segment (start 66.42 47.76) (end 66.42 48.26) (width 2) (layer B.Cu) (net 1))
  (segment (start 59.01 40.35) (end 66.42 47.76) (width 2) (layer B.Cu) (net 1))
  (segment (start 66.04 30.48) (end 66.04 38.1) (width 2) (layer B.Cu) (net 2))
  (segment (start 60.96 25.4) (end 66.04 30.48) (width 2) (layer B.Cu) (net 2) (status 10))
  (segment (start 69.85 41.91) (end 66.04 38.1) (width 2) (layer B.Cu) (net 2))
  (segment (start 76.2 41.91) (end 69.85 41.91) (width 2) (layer B.Cu) (net 2) (status 10))
  (segment (start 53.5 25.4) (end 53.34 25.56) (width 2) (layer B.Cu) (net 2) (status 30))
  (segment (start 60.96 25.4) (end 53.5 25.4) (width 2) (layer B.Cu) (net 2) (status 30))
  (segment (start 53.18 25.4) (end 53.34 25.56) (width 2) (layer B.Cu) (net 2))
  (segment (start 44.64 25.4) (end 53.18 25.4) (width 2) (layer B.Cu) (net 2))
  (segment (start 93.98 30.48) (end 88.9 30.48) (width 1) (layer B.Cu) (net 3))
  (segment (start 83.82 25.4) (end 83.82 27.94) (width 1) (layer B.Cu) (net 3))
  (segment (start 86.36 30.48) (end 88.9 30.48) (width 1) (layer B.Cu) (net 3))
  (segment (start 83.82 27.94) (end 86.36 30.48) (width 1) (layer B.Cu) (net 3))
  (segment (start 86.36 20.32) (end 78.74 20.32) (width 1) (layer B.Cu) (net 4))
  (segment (start 78.74 20.32) (end 76.2 22.86) (width 1) (layer B.Cu) (net 4))
  (segment (start 76.2 22.86) (end 76.2 25.4) (width 1) (layer B.Cu) (net 4) (status 20))
  (segment (start 93.98 27.94) (end 88.9 27.94) (width 1) (layer B.Cu) (net 4))
  (segment (start 88.9 22.86) (end 86.36 20.32) (width 1) (layer B.Cu) (net 4))
  (segment (start 88.9 27.94) (end 88.9 22.86) (width 1) (layer B.Cu) (net 4))
  (segment (start 43.18 48.26) (end 48.26 48.26) (width 2) (layer B.Cu) (net 5) (status 30))
  (segment (start 48.26 48.26) (end 58.42 48.26) (width 2) (layer B.Cu) (net 5))
  (segment (start 33.02 48.26) (end 27.94 48.26) (width 2) (layer B.Cu) (net 6) (status 30))
  (segment (start 27.94 43.18) (end 20.32 35.56) (width 2) (layer B.Cu) (net 6) (status 20))
  (segment (start 27.94 48.26) (end 27.94 43.18) (width 2) (layer B.Cu) (net 6) (status 10))
  (segment (start 36.64 32.72) (end 38.18 34.26) (width 2) (layer B.Cu) (net 7))
  (segment (start 36.64 25.4) (end 36.64 32.72) (width 2) (layer B.Cu) (net 7))
  (segment (start 36.64 25.4) (end 20.32 25.4) (width 2) (layer B.Cu) (net 7))

)
