(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "VCC")
  (net 5 "/SENSE_LOW")
  (net 6 "/SENSE_HIGH")
  (net 7 "/SENSOR_TRACK")
  (net 8 "Net-(R4-Pad2)")
  (net 9 "Net-(R12-Pad2)")
  (net 10 "Net-(R10-Pad1)")
  (net 11 "/OUT")
  (net 12 "Net-(C7-Pad1)")
  (net 13 "Net-(R12-Pad1)")
  (net 14 "Net-(R13-Pad2)")
  (net 15 "Net-(U2-Pad9)")
  (net 16 "Net-(U2-Pad6)")

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB) (tstamp 1401a68c-ab73-4f17-b7fe-ecafc0e1330f)
    (at 104.14 39.37 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/cf81db3c-aa4d-45ee-8299-1881e46e25b3")
    (attr through_hole)
    (fp_text reference "J1" (at 4.385 -2.27 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce0fe750-e847-49eb-b719-26932e004227)
    )
    (fp_text value "Conn_01x03" (at 4.385 7.35 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c85a4489-eaf0-46de-a1bb-cfd43db20f22)
    )
    (fp_text user "${REFERENCE}" (at 2.77 2.54) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 27498e76-8756-484f-8bad-f990d2fe8b81)
    )
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer "F.SilkS") (width 0.12) (tstamp 0615247c-4c98-486b-9582-bdda79652462))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer "F.SilkS") (width 0.12) (tstamp 0b45ddae-c393-4628-9f80-fee65129a8b3))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer "F.SilkS") (width 0.12) (tstamp 10131e1a-69fb-4d91-b12e-c472c48a2120))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer "F.SilkS") (width 0.12) (tstamp 164d01e1-8a06-475e-8323-20273cb6e7ce))
    (fp_line (start 1.44 6.41) (end 4.1 6.41) (layer "F.SilkS") (width 0.12) (tstamp 1a9a0a4a-346f-4f72-8090-030a53cd6c97))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer "F.SilkS") (width 0.12) (tstamp 359df499-c39d-463d-bc5c-996729cb9ff4))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer "F.SilkS") (width 0.12) (tstamp 3a121826-8e98-4a1f-b55b-cd55b344831e))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer "F.SilkS") (width 0.12) (tstamp 561eedc6-ce51-475c-96ff-bb5796153e3f))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer "F.SilkS") (width 0.12) (tstamp 57277fc1-7014-4089-9c36-1c331c49d984))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 77218962-dda7-4207-9635-2b038cd2ae8e))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer "F.SilkS") (width 0.12) (tstamp 849667d2-aad8-4c28-a6f7-8f019f006d4a))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer "F.SilkS") (width 0.12) (tstamp 870d8ccc-84e3-48d0-bda5-2989c760dc54))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer "F.SilkS") (width 0.12) (tstamp 8c0a088c-4294-4bf0-b1c6-47560ba07d1f))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer "F.SilkS") (width 0.12) (tstamp 9079f328-4450-4647-adf5-37bc38fe47de))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer "F.SilkS") (width 0.12) (tstamp 96020141-0751-4646-99ab-8d499b240da9))
    (fp_line (start 1.44 -1.33) (end 1.44 6.41) (layer "F.SilkS") (width 0.12) (tstamp aa8ebd18-c74b-4bf3-926c-85499cd31a91))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer "F.SilkS") (width 0.12) (tstamp bd8435ec-9fce-4241-a39e-b2adc0893175))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer "F.SilkS") (width 0.12) (tstamp be8c535a-efef-4cf5-99e1-9429355cd442))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer "F.SilkS") (width 0.12) (tstamp c1bb6ff6-413a-4c97-8406-c240141247e2))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer "F.SilkS") (width 0.12) (tstamp c49d213a-4601-4d64-b426-6f0eb3dea2e6))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer "F.SilkS") (width 0.12) (tstamp c6e13f81-1336-448f-ba69-b78e5296f3ea))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer "F.SilkS") (width 0.12) (tstamp c6ee59a7-1e39-4aa2-8d50-92254e5cc96e))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer "F.SilkS") (width 0.12) (tstamp c79fb6ec-feba-4645-afd1-7396ba4f9c93))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer "F.SilkS") (width 0.12) (tstamp ce168e2a-252c-4432-9e1f-cc7df082e26d))
    (fp_line (start 4.1 6.41) (end 4.1 -1.33) (layer "F.SilkS") (width 0.12) (tstamp e29945ef-5971-46d0-a426-94da592eede7))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer "F.SilkS") (width 0.12) (tstamp e3acd025-026d-4100-9a12-dea4312ceb18))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer "F.SilkS") (width 0.12) (tstamp ed61eac3-73a8-409c-b768-f2ce280f5b28))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer "F.SilkS") (width 0.12) (tstamp f14cfb9a-ca19-4b90-89f9-589558447894))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer "F.SilkS") (width 0.12) (tstamp f637c8c8-4a9c-4d20-9d91-e56bd1a43e5a))
    (fp_line (start 10.55 6.85) (end 10.55 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 1310ab5d-0f70-4f35-88e4-cf32e0666db0))
    (fp_line (start -1.8 -1.8) (end -1.8 6.85) (layer "F.CrtYd") (width 0.05) (tstamp 3cf7d7e7-1670-42ac-8aa6-4de84def7b60))
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 57c55535-be9c-4d86-aa10-3160b1639f17))
    (fp_line (start -1.8 6.85) (end 10.55 6.85) (layer "F.CrtYd") (width 0.05) (tstamp ea1aef42-56c8-4fa8-9531-abfcc69d25a1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer "F.Fab") (width 0.1) (tstamp 03e2003a-f8f9-4285-824d-440200d6c42b))
    (fp_line (start 4.04 -1.27) (end 4.04 6.35) (layer "F.Fab") (width 0.1) (tstamp 1ed5a4d5-eed7-4297-b16c-0356720c02f8))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer "F.Fab") (width 0.1) (tstamp 23edfaa9-51c0-42c5-9139-aecfee36342e))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer "F.Fab") (width 0.1) (tstamp 384178f7-8884-4a95-8dbf-73a03bad7658))
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3dc66241-36ed-4a04-9bb9-a035b3e7e7a9))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3e2c1985-6270-4244-9585-0981de6fe5b1))
    (fp_line (start 1.5 6.35) (end 1.5 -0.635) (layer "F.Fab") (width 0.1) (tstamp 4a5ce650-6e3a-4eba-90af-0d4f24b28574))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer "F.Fab") (width 0.1) (tstamp 553fedc8-126d-43dc-b606-c361cc6db244))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer "F.Fab") (width 0.1) (tstamp 554a2d78-c0b7-4570-b5be-eaf3f4bcf744))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer "F.Fab") (width 0.1) (tstamp 65697ac5-0dc3-4167-a811-19cecf503ae4))
    (fp_line (start 4.04 6.35) (end 1.5 6.35) (layer "F.Fab") (width 0.1) (tstamp 65ab0377-04c8-457b-96fc-52d6c736299d))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer "F.Fab") (width 0.1) (tstamp 6663883b-7567-464f-8f1e-9b18cfaab149))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer "F.Fab") (width 0.1) (tstamp 6a446ae8-e516-48da-8e1c-0d95dff9b3a1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer "F.Fab") (width 0.1) (tstamp 7429bd53-9b35-40b1-bf72-65b57c9b93f7))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer "F.Fab") (width 0.1) (tstamp 7b95830a-c57e-40c6-ae42-da618807c01e))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer "F.Fab") (width 0.1) (tstamp 84006e4d-868c-48fd-b79b-19351a9c9aaa))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer "F.Fab") (width 0.1) (tstamp 8ddd1ebf-e6a3-47a0-9898-1a97c484ab2d))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer "F.Fab") (width 0.1) (tstamp a92a0c4d-798a-41aa-bab6-351a7615d4b6))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer "F.Fab") (width 0.1) (tstamp b07f722c-5bad-4e63-912a-06cd2f123780))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer "F.Fab") (width 0.1) (tstamp c39a75ea-e3da-4978-a49f-5a8d4011a1cc))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer "F.Fab") (width 0.1) (tstamp d3adcddc-9b28-483c-964b-e7b78898c9cd))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer "F.Fab") (width 0.1) (tstamp e4e1a51f-8e71-4ada-83c8-fa5060827c8c))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer "F.Fab") (width 0.1) (tstamp fbf0d1f0-25c5-4e84-a788-b88fb59b1237))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 2b27309b-5575-41a8-8e30-62e332d976d6))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/OUT") (pinfunction "Pin_2") (pintype "passive") (tstamp 9d28ffef-f253-4bce-9ac9-0c94e25ddd2e))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "Pin_3") (pintype "passive") (tstamp 19c0a43d-8ad7-4328-9e0d-5f6e52bfcebd))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 14f4fa55-a477-4365-a730-bbb604543dbd)
    (at 139.89 50.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2b17d")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 579e9775-0d39-45b5-9c43-f5be39738637)
    )
    (fp_text value "10k 0.1%" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 514e1e9c-ee83-45e4-a558-ae12f0a3f1f4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 55cbe8b0-9229-46f2-b7ca-4aa6780b527d)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 574babd2-c80f-4d1c-8780-7aef71de6901))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp f31ddb02-22c9-4fb5-aa93-fb0436c23dd7))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 0544b1d2-cd81-4330-a214-45846056cde5))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 24f0f170-ac92-4577-9d27-192dcf760dcc))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp a66cde9b-41c1-4269-a9d8-05f60b6e8d6c))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp e46acfdc-3f6d-48d3-9629-5b9de774f67c))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 1f21596c-fbfd-4b7d-843e-3125a4cccbd2))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 47e5370c-2f1f-4f08-b477-c901c8655fcf))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 8f7e483f-d43e-4883-9a61-b3958a64d3f0))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp acecd75e-5763-4905-a3d4-9c0d19021a50))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R10-Pad1)") (pintype "passive") (tstamp c242c664-170e-4bbb-8c19-833d335c395d))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 276a2794-2884-4ac8-b00f-7e93aac8b824))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 16e8683a-9fee-42a1-866a-a8f9252db5b2)
    (at 149.84 47.05)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d222f8")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp afda18e5-070d-4f98-8fdb-44eb6d1e9fde)
    )
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0eed7bcd-ba64-4dfa-825e-fbb9d6143674)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 97a0b033-fe3a-4d45-a39a-daf01af4d26a)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 63a03c7b-13fe-4bee-a853-55c358e4f47d))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 734980f3-f0c6-4271-875b-f1b6820e922c))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1b56379e-2473-4a2c-b185-cc5274dc5b6b))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3ac763d8-634a-4721-8453-4eb07ef626d6))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 446c254c-3f3c-45b3-8820-cef98e341970))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b79aa3c0-704c-48d5-a124-e17a003fabb0))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 72ca54e0-b284-429a-b82e-5cf1f5ae7fae))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 8223ddf0-4e22-4ac4-bf1a-38ddc0114dfa))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp e4adcb80-9b11-42f4-a539-b9b3848f0f7d))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp ebffa8a3-7d55-4647-b9fe-95933f0bbd19))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp c31f2019-f738-4afd-b131-ced484c1e707))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SENSE_LOW") (pintype "passive") (tstamp b54b528f-0f58-4f0b-b85c-bc9dd826e910))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 179856c2-8fd2-4d2e-9d67-b9f49663ccc6)
    (at 134.04 60.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d22484")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9d3972b2-ca77-4404-ad3c-c6d0e8c8a969)
    )
    (fp_text value "1n" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f418cd9-2ce3-4bac-82dc-0c3c989b010b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp d87f7154-1f22-4f26-914b-8de70411c424)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 09296c51-1def-4e22-b96c-8bac6d773704))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp f46991e4-0d24-432e-be1c-04d1f9997afd))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3cbb1b7f-f712-411a-81bd-da089228946f))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9ab8d96c-cf60-416b-bf9a-3fea8c0c2d0a))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ce28b351-775b-402e-a251-4c9600710036))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp fc0f0d81-bb88-4fe0-babb-034c6235b930))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 0bfc3b94-d1c6-45d4-a683-0d22bac69da2))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 3f8e5603-e98c-47bf-b668-6ead760b202e))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 7818d365-4d03-44ab-b838-90fbbb061b79))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 9379f832-4b7a-4194-81ab-351596317cdf))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SENSE_HIGH") (pintype "passive") (tstamp 53808d03-d87d-419b-959b-00b8f6038df6))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 8ce51c6d-a9cd-411b-ad06-e0c70eb0e632))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 1ca73b79-2e8d-4af1-b3a0-94cdb6be099a)
    (at 135.54 55.92)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2b42b")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 86947626-bfb6-49ac-a255-af7cab975952)
    )
    (fp_text value "10k 0.1%" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5f67ddde-30a6-4339-a9e0-15e71e1d3263)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp f881e732-34aa-4945-b677-3c5d949bfb35)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 81b83c63-06a6-4e1c-9ac8-d2606deb1c1b))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp eb8398f8-1741-4447-aaa7-99c7debf7c49))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1dc6a066-e4d0-404a-b338-e220192eeafc))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3675debd-4cef-4ba4-9659-9188fb800ee8))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 55231948-ffd6-49f0-9050-8e79272c760d))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 968c27b2-5800-4663-ba24-2c9794038dfd))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 15efb9cd-ef76-4a67-9781-544533d4c6cb))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 23c4ce42-d8bf-4881-a790-e416979d985d))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 9855c2b0-af20-478d-92b4-77ee0158856b))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp e9730335-bce1-4cef-b748-d13f17e22007))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R12-Pad1)") (pintype "passive") (tstamp b95aa0dd-80dc-4ee2-9ea6-d79cd316b590))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(R12-Pad2)") (pintype "passive") (tstamp aad2a30f-860a-49a0-b1f1-e80f6fc85294))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 3e149755-5c16-4459-8376-b4e97b59898d)
    (at 135.54 53.41)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-00005514275d")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b22c2529-bf3c-4a9e-9b2a-11c1bd6ebdec)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7bc09c9d-d9e6-4713-b790-d43e4cb6261f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7f14c2a4-6551-4309-a5d1-3e5d4e3e9a48)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp e456543e-e104-4fbe-a5a6-94c3369a934e))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp ee98b24b-0809-4d27-a263-d656ac4f1461))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 39175dcf-ce59-49dd-bf43-22eb32f967e8))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp a0ea4d3b-d969-42de-a19b-97eb49f03856))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp a2f5dcae-75e6-46a8-972c-1facdb1e6e70))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp cc9f9529-c8dc-4e20-a858-8a86ee9ca2c0))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 1b8ace64-deec-48fb-868b-be6fd9b9515a))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 23ee2b18-739b-4a13-8e5a-c64e9cd32cc4))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 28f4c1ed-7166-4d37-ab91-a68d2a359847))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp d8bf4876-e485-459d-b9fa-01b16439602e))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C7-Pad1)") (pintype "passive") (tstamp cc65a967-ffd2-492e-8c20-a99bfc6773a0))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R12-Pad1)") (pintype "passive") (tstamp 43663ad3-fde1-48fc-a4d2-d8b3c6a6647a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 4dec2c44-482d-430f-9dd6-8a22534e7ed9)
    (at 144.24 52.07)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d22174")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f335bd86-648d-4461-a2e1-94cb310869bd)
    )
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 68d917e2-53c2-4a69-8ed2-7983f0630bc9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 8dcb25f1-7581-4b3b-8e4c-3d387477a48b)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 7d5c3d4b-d015-4896-b07b-4fe2f86bae0c))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp a7cf764c-26aa-4a3d-b24b-73b2d95ec172))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5ea7c933-739a-4215-a81f-fedbc84898ef))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8692ac02-eb08-45df-8a1e-5daa047ca1eb))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9a218c7d-97e8-449a-90fd-9d65671398c3))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp c20966ef-758b-40be-80fe-e894a6e31bab))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 0a708d83-24ac-4dd0-ab73-a7bb3a82297f))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 48897115-58ca-42a2-8521-22c420b55740))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 65641b02-4f44-4370-8377-aef165fd4fc5))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp dee4e39d-4509-4477-a348-58b71c7b6ad5))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SENSE_LOW") (pintype "passive") (tstamp 88eda6fc-f1a1-4563-8f3d-37dbbde24720))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pintype "passive") (tstamp ae0e8eba-3399-45be-baf0-834bb0b400bd))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 66d6754a-2898-4fb8-aff8-ac41bc61ab1c)
    (at 129.69 60.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2b156")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8b0bec82-62a2-472a-9afb-fd907505c41d)
    )
    (fp_text value "10k 0.1%" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0caab1bb-5acc-4081-8d4b-75db7b9f6b5a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp a62f017a-20bd-4939-bf00-b24be59eb405)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 2b9f4b30-91e1-4437-ba31-96f9b899876c))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 94220278-318e-4b5e-a47b-36652d2e90e5))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 21863b39-c8f9-4731-9671-aba839129eba))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 759f0f8a-1df3-4b64-9d20-0bf56740d0d3))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b7c88c59-6c59-4320-90a7-7122beeb1a80))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e0902e4f-fccd-4b70-9252-b1c625cb8192))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 46ff9576-91e9-4146-be16-3aaa24991710))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 5c5665de-d35d-4fb2-835b-cf4fe42f1427))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 7496b592-cb95-4893-a532-dcaf365ece39))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7f931cac-c047-41c7-87bf-3a671f6a7688))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R10-Pad1)") (pintype "passive") (tstamp b0cae1d3-35fa-4b7c-a1dc-e6841ab58ea5))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U2-Pad6)") (pintype "passive") (tstamp 7758c6ad-75a3-4a9c-887b-1e7a1ffb1f6f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 66dea9dd-eed6-4d0c-b869-5f209502a55a)
    (at 139.89 52.91)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2428c")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 86a6d0b8-5a96-4623-ac10-e10135c1983d)
    )
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9bd40f53-6e1d-4dee-b8b8-f4b22d979e94)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp a51173d4-d329-416f-9557-027c028b2758)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 221446a6-beb3-4f78-a25a-383b41cb80cd))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 7f96842d-2d7e-4476-bbe3-9516b26a63c7))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 03795f41-671a-4144-bf04-b8eacb977de0))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 28674873-f653-4c84-a95d-de07e16831c0))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4c6175fd-1416-4289-9607-4d4667102d4a))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 69ab88b5-ac28-4630-9750-29b6a410fd5d))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 3bf9a07e-b37e-4372-80ce-d7ebff95e13a))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 95d2f6a9-aaf0-47b8-85bd-f3a378f6b876))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 9a2c60d1-737c-4e8c-815c-44f57b7fbd75))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp eea6c813-35aa-4208-9679-4c3e132bfa73))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pintype "passive") (tstamp b9a4c506-9b6e-4b0c-9ad0-4c6de6d8c1bd))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 1d72717b-23d1-4ec0-a4da-0426758671ef))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 682be152-0949-4648-ba6e-c90519c90ed2)
    (at 139.89 55.42)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2222a")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 441d39f6-906d-4117-b6ab-36681471e794)
    )
    (fp_text value "1n" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c330e04-56e0-46ec-b228-80d8120ab8ee)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 615bfcbb-9fdc-4ac3-bb55-b2ecdd507232)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 083890da-4717-4674-aecc-14ce111b4829))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 6130f023-f64d-4b38-9ee4-63fa48b8685b))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp c54baf95-de38-40fb-886a-286b313e9d03))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp c55c4157-e42e-400b-9997-01c2d28dcd3a))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp d447e240-1a93-40b4-a3b0-c9c7f93fa000))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp eafc360f-3971-4618-b08b-04e67aea6242))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 06598b7d-7c1e-4cb4-a493-4a03491d2645))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 367bcc4c-e916-4a37-9b0b-8ed2a3151dd4))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 5dbcd0f4-1917-4239-8634-4fa4b353f0c3))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 8fc8a325-21a6-4411-90a9-08ca29e22fe0))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SENSE_LOW") (pintype "passive") (tstamp 276ef1b3-8036-4517-9d80-76af7d4d59f2))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 270b872c-3fb6-4ddd-a668-7918433088da))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 74ed4840-a4b7-4a06-b90c-22f031b7f574)
    (at 139.89 57.93)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2193d")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fb37e45f-da12-4bb1-99a9-574c01cb05ab)
    )
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96133194-2128-4253-88c6-16addf8a1f41)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7f76a753-5f16-4842-9a19-ee2f6ddf8e19)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 67a577c0-df05-4dcc-a16d-e8c783996f4f))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp d5928262-5955-4ace-ada7-a2163ef9f265))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 385210ee-36a6-4a86-ab3d-3c5e6a8f517d))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 55e38bfb-3b3c-49b9-b4c9-8b490397a7b4))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 631972f1-71f1-4f0b-a38f-2e8293a4c29c))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f8b33451-0591-4efe-a228-e52f69b6baaa))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 2dc9f45f-e2fb-453e-ae20-80d30cfdd574))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 2f4cf4c5-e8e3-4757-be60-42208d52aca1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 5ce79988-2e11-4165-9263-50d16d5867a0))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp abe73efb-de1f-490e-b141-2b5b54c07bb0))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp ec6e53f7-eb69-45ae-a33e-61491393ae14))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (tstamp f5986cd7-b226-4410-b370-8ab8ded03df3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 8477568c-1490-475a-9eb1-e66e3ed5051d)
    (at 149.84 49.56)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2209d")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f94c563-0ba9-46a1-a527-254acfd0e69b)
    )
    (fp_text value "330" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3f271c83-9e32-4421-9bea-d3a71840a9c6)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 4d566c0f-ca8c-4243-83a7-219f2fb324b0)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 346bfaa0-536b-46d2-933d-ea9d03593730))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 55803e58-b2b4-449a-bade-2d1f0ab4e253))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1afe4e8b-6725-45f3-8238-161bcf997427))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 58a59408-5766-4926-9d70-4b5af4ffcc34))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp af0fce2c-0e75-492f-ae28-2f98b12bebec))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp b3cb8598-bdd2-41e2-b013-adfb154182af))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 06dab9a4-36ea-4aa5-9f7a-68edc3df3ff3))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 8a861d40-6f66-4b5a-aeb3-f02babbcd915))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 96169d1c-7098-4d4a-80c3-750a559b519e))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp d54c6ad5-bc4c-4853-9dbf-d663aec3ea7e))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/SENSOR_TRACK") (pintype "passive") (tstamp 71e0d008-aa01-4edf-9c3c-6df48d1dcd34))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(R4-Pad2)") (pintype "passive") (tstamp c09777aa-8a30-409a-9fb3-9f301d9f9c26))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 8f2d931d-1d6c-478f-aaec-734d0d23a332)
    (at 144.24 54.58)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d21e5c")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8bc780be-65f7-4b6d-af78-abba3ceb7d99)
    )
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b27e732-3df9-4bfa-a6d4-22fc53645d7e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 0503f3f4-df54-4163-8517-8c24651443d3)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp dff1e449-e365-4829-b697-c38af6ffce28))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp f772055b-2849-4fb1-a753-1870bcd087cb))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 21623e6f-4723-4d58-9e22-9d1bfea84d8d))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 27752368-ac83-4d50-99cf-e5954dad23a3))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2aea46f1-2f3e-47d4-bc52-2a20af046d80))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 67b8a3d0-fc98-47a8-b860-27a7c2ac4247))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 7929f616-68fc-4319-8e57-cd1650bad44a))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 97527093-a065-4cf9-8d71-a0365854b84b))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp d7ce9b95-3005-4fc0-bceb-7ff4c699be93))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp e8c423cd-cb42-41fa-9caf-b1caa892089b))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pintype "passive") (tstamp 7feb9ae9-e42b-449f-b9e1-92bb7a22b96e))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 5f9a6b24-f667-482e-94d7-24052a47a4d1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 95c993cb-b773-40f8-bd6f-15165d39ad40)
    (at 119.24 65.05)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2252c")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d4b07498-b176-4834-833b-60f46d9885d1)
    )
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ba3b3a86-c3e1-49ff-a32b-00b48aa8dd6d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 208bdbc0-2442-4981-bb62-1f80dfa03751)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 4ddb00e8-7e18-4f10-91f5-d2012f0bdf62))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 7a7176d0-bd32-4e12-b06a-03b0a9e4a0a0))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 08a210c1-3999-4516-aa51-593d352b8af5))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4f9aaa9c-bc5f-4582-8569-337371fe3b13))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 911f57cf-ffe6-4181-b5c2-79ea51b530b8))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b6b04c42-17f8-45bd-a9d0-480673242f37))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 6db4f041-d515-4073-ad7c-7dcb312f128a))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp baf154d2-0894-4642-af2e-0ab889a9a2f5))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d2483a62-c44d-464e-8a63-ea80d313feac))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d92423b4-0b5c-44fd-be20-004192fedb96))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SENSE_HIGH") (pintype "passive") (tstamp 26ae8cbf-adda-4470-8eca-449955350227))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pintype "passive") (tstamp 77e8614a-66b7-4870-8a68-8773bb88ce0d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 9663fd20-306a-4ddb-bb60-95699e12c258)
    (at 135.54 50.9)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000551434bc")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6c4fbc0-2810-4b41-913b-5fa930513851)
    )
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 79a79f3c-0810-4450-a437-e68532e0ab20)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 9f17bc8f-31b4-4383-a353-c73aca3e0804)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 93c82d62-509d-41a7-8554-692280a4f403))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp cc8585d7-4652-4fc8-b393-52ed2f56afeb))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5087090b-07fd-48af-aa5b-c6d2d74767c3))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 85d0d654-c0c7-4dc2-8244-e4e471efc343))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b150798f-e837-47c8-86df-cd034b23c95f))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp f7c1ab33-539a-4dd9-80dc-5a8b5f05d765))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 3c44f177-7e82-4280-b256-3f2684e18bf0))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 77a74abc-fcfe-40fa-85ca-f140cf1d9793))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp c66b7dd1-8fe9-4be7-bdfa-9e84a5061d19))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp f382b03c-f97b-4828-b9aa-beea2e4aebd9))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/OUT") (pintype "passive") (tstamp b1ecfd8a-762d-4507-9712-5afcee31616f))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 9cbc2d66-07f4-4f77-81cf-931c1170ce42))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 9b0850cb-82e9-4c3d-8997-2bdc1cc45d7f)
    (at 123.59 65.05)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000551427db")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3ab5ac1d-ef1a-4b56-801c-edfbb672b990)
    )
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f5722f12-566c-4ede-96d3-b6e6c41e1120)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp ba6702c7-9891-4315-a745-4470a6e95967)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 1a1d2e05-223a-4eb7-8b3f-d103370a1ee4))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp c91205d9-201a-470c-a1e4-a44abf3e97fd))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4c9fcc59-3901-4891-910c-7b4e709feef2))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 651ff3da-3fa2-4bd8-928f-1480fdd74a5e))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp a2841d5e-566d-48d0-946a-746772d3799f))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp c09c9933-7a8c-4d47-b024-6ffccdd70813))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 037f13f9-bdcc-42cf-a43c-43e1886479b1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 3eb7200c-4910-4b44-8e77-ac82eb16d67c))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp bd6d9b04-0ce4-49be-8862-fe921de1f132))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp e3187977-8ef7-4b62-ab7a-b4ce03142569))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C7-Pad1)") (pintype "passive") (tstamp 912a5d72-b4d3-457d-8ca3-f3646b5a9d0b))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 5e8a99a0-a30e-447c-956a-a4cc9d125d2f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp a16476b0-2612-4ebe-b86e-dff2d7f0f0f3)
    (at 138.39 60.44)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d218de")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d5465150-5339-4660-b177-7c675cd4e397)
    )
    (fp_text value "18p" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2c280d6f-d02f-4c57-b38b-86e28371340b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp e2d71709-aabf-4108-8d54-b83062214a0a)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 1dbf6911-0d7b-4a7f-9bca-ef9b1c544f8b))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 94531610-e773-4054-83c6-0ddcca51bae2))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 56b6855e-a3dc-4f66-84cd-7c7036117591))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 84d5269c-9614-4818-b445-086c67b550e0))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp a77b0ff0-eb02-4a0a-b452-bb4f3dfae9f3))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b8f86d21-1ad1-4bb4-bed6-945ffd9fbecb))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 09008b1d-3488-4448-b80f-79ace5e2021c))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 32a9d669-7755-4874-bad6-5a9ca3feddc0))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp d61906b1-b5ed-41f0-95a7-798773ebc0da))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp fb830e2c-a9d2-45f9-8a23-0acf410b0498))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp 1f24632c-7a8c-48e6-9530-34bef1fb50d9))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 4338717b-9b7a-4cb5-87c7-d1c9975615e6))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7) (tstamp a1d82332-d4de-4749-9c0d-6a1e572d749a)
    (at 140.44 47.47)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d21fcd")
    (attr smd)
    (fp_text reference "D1" (at 0 -2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 85021155-e4c6-4e5c-a65e-272ecfed25b6)
    )
    (fp_text value "DIODESCH" (at 0 2.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1a7556c5-478b-4fb2-aab0-1b619c3578c8)
    )
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 819aac9a-df3c-4311-a3a6-feaa69716d02)
    )
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "F.SilkS") (width 0.12) (tstamp 7ea5631c-5b33-44e9-ad69-b426d616fd98))
    (fp_line (start -2.25 -1) (end -2.25 1) (layer "F.SilkS") (width 0.12) (tstamp 88e04a41-e4e2-458c-95fd-3e2c2fb6edb2))
    (fp_line (start -2.25 1) (end 1.65 1) (layer "F.SilkS") (width 0.12) (tstamp f23148cf-ecb5-4392-af6b-fc9d1ddeef78))
    (fp_line (start -2.35 -1.15) (end -2.35 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 1452e9b3-5165-417a-982d-e4187beffbb7))
    (fp_line (start 2.35 1.15) (end -2.35 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 2dcea4ed-93e3-43d3-93f5-682233a1f54d))
    (fp_line (start 2.35 -1.15) (end 2.35 1.15) (layer "F.CrtYd") (width 0.05) (tstamp aae03c17-3899-4a78-a2f7-b86232b274b9))
    (fp_line (start -2.35 -1.15) (end 2.35 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp e5481c5b-d62c-48f5-b3c0-0efa6f33d773))
    (fp_line (start 1.4 0.9) (end -1.4 0.9) (layer "F.Fab") (width 0.1) (tstamp 0d267438-0193-44f3-865c-accc4234be43))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "F.Fab") (width 0.1) (tstamp 165c0e7e-9ec8-4308-ac85-38e5f75c3df6))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer "F.Fab") (width 0.1) (tstamp 21b67521-a8e5-43a0-aaed-b65e9eebd538))
    (fp_line (start -1.4 -0.9) (end 1.4 -0.9) (layer "F.Fab") (width 0.1) (tstamp 54c575fa-bbac-4b53-b918-ecb02b923235))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer "F.Fab") (width 0.1) (tstamp 78652582-ad3e-4f6a-a344-6df08f4cc8a9))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer "F.Fab") (width 0.1) (tstamp 8cc27dd4-ed68-4ea7-9a44-6cf7eb647a67))
    (fp_line (start 1.4 -0.9) (end 1.4 0.9) (layer "F.Fab") (width 0.1) (tstamp 91c9444f-3879-45d6-b9f7-c5f4df745e92))
    (fp_line (start -1.4 0.9) (end -1.4 -0.9) (layer "F.Fab") (width 0.1) (tstamp d2b227f3-35df-4d45-825b-98153f041e51))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "F.Fab") (width 0.1) (tstamp db61d98c-2721-4697-b5eb-fe30c760189b))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "F.Fab") (width 0.1) (tstamp e7bc3e88-a9fc-4339-a449-4714da05b998))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "F.Fab") (width 0.1) (tstamp ec1780b6-0fd9-419a-951b-78d04c732239))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/SENSE_LOW") (pinfunction "A") (pintype "passive") (tstamp 38634f3d-b1e1-4a82-b0c4-9532c8906c1a))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/SENSOR_TRACK") (pinfunction "K") (pintype "passive") (tstamp 64129a38-4607-4ed7-a043-65e6382eb022))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SO-14_5.3x10.2mm_P1.27mm" (layer "F.Cu")
    (tedit 5EA5315B) (tstamp ab2f0e38-6f26-4b86-a6fe-bb9e1e4097e4)
    (at 106.68 50.8)
    (descr "SO, 14 Pin (https://www.ti.com/lit/ml/msop002a/msop002a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2af04")
    (attr smd)
    (fp_text reference "U2" (at 0 -6.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 972ee5b5-4ebf-4571-a609-b2ff379f4176)
    )
    (fp_text value "LM224" (at 0 6.05) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 17fb13da-832d-495c-9c74-36719f2b4810)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9082bbc1-25bf-4fde-a66b-4f0665fd500d)
    )
    (fp_line (start -2.76 -5.21) (end -2.76 -4.37) (layer "F.SilkS") (width 0.12) (tstamp 1137ee6d-dd40-4519-96fa-6c43089e1d1a))
    (fp_line (start -2.76 5.21) (end -2.76 4.37) (layer "F.SilkS") (width 0.12) (tstamp 26a1b36b-1219-4c80-925c-a9c5058b491e))
    (fp_line (start 0 -5.21) (end 2.76 -5.21) (layer "F.SilkS") (width 0.12) (tstamp 278a864d-023c-43eb-851c-6913f9252643))
    (fp_line (start 0 -5.21) (end -2.76 -5.21) (layer "F.SilkS") (width 0.12) (tstamp 31f5332a-cda1-44df-8403-3e68b87901af))
    (fp_line (start 0 5.21) (end -2.76 5.21) (layer "F.SilkS") (width 0.12) (tstamp 3ad499f6-57f6-4c8c-85ce-3125ccb91ac5))
    (fp_line (start 0 5.21) (end 2.76 5.21) (layer "F.SilkS") (width 0.12) (tstamp 3c256267-ba56-41cd-bc28-c78a1beee726))
    (fp_line (start 2.76 5.21) (end 2.76 4.37) (layer "F.SilkS") (width 0.12) (tstamp 8d859913-6565-4cba-a03d-d7acbcee9d46))
    (fp_line (start -2.76 -4.37) (end -4.45 -4.37) (layer "F.SilkS") (width 0.12) (tstamp c920e409-99fa-4407-b2a3-df44ae7a5073))
    (fp_line (start 2.76 -5.21) (end 2.76 -4.37) (layer "F.SilkS") (width 0.12) (tstamp cafe40a4-c58c-42f3-b29b-7c402bd48533))
    (fp_line (start 4.7 5.35) (end 4.7 -5.35) (layer "F.CrtYd") (width 0.05) (tstamp 1b1a09ca-2161-40fc-8e2a-c29cd06f69a6))
    (fp_line (start -4.7 -5.35) (end -4.7 5.35) (layer "F.CrtYd") (width 0.05) (tstamp 3b7dd1c5-7bd3-43c4-a1b5-a503f4d678d0))
    (fp_line (start -4.7 5.35) (end 4.7 5.35) (layer "F.CrtYd") (width 0.05) (tstamp 77003b90-9142-4f25-b2d4-01d7fcbc2d88))
    (fp_line (start 4.7 -5.35) (end -4.7 -5.35) (layer "F.CrtYd") (width 0.05) (tstamp 7c28910d-9472-4e12-b71f-f36b12b04564))
    (fp_line (start -2.65 -4.1) (end -1.65 -5.1) (layer "F.Fab") (width 0.1) (tstamp 68fc527a-7ab7-43d9-a5dd-9cba5f4f0d47))
    (fp_line (start -1.65 -5.1) (end 2.65 -5.1) (layer "F.Fab") (width 0.1) (tstamp 90336d97-01b1-431a-9a78-e9a6bba4c3e7))
    (fp_line (start 2.65 -5.1) (end 2.65 5.1) (layer "F.Fab") (width 0.1) (tstamp 9fd2f091-27b0-437c-9632-a66a949056de))
    (fp_line (start -2.65 5.1) (end -2.65 -4.1) (layer "F.Fab") (width 0.1) (tstamp cf6de12c-4b57-4ae6-b64d-717e52dd76ac))
    (fp_line (start 2.65 5.1) (end -2.65 5.1) (layer "F.Fab") (width 0.1) (tstamp ded074b5-99af-40b2-a0b7-661c6e825165))
    (pad "1" smd roundrect (at -3.4625 -3.81) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R13-Pad2)") (pintype "output") (tstamp 2e3308da-3ba1-48c7-92de-f98c0c9e2339))
    (pad "2" smd roundrect (at -3.4625 -2.54) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R13-Pad2)") (pinfunction "-") (pintype "input") (tstamp b71ba786-e47b-42b1-a115-425dc8d0e49a))
    (pad "3" smd roundrect (at -3.4625 -1.27) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C7-Pad1)") (pinfunction "+") (pintype "input") (tstamp b9908683-1811-4aab-a2d0-9d5d0dc585eb))
    (pad "4" smd roundrect (at -3.4625 0) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "V+") (pintype "power_in") (tstamp e5fe0654-a9a8-4493-a280-1f15903c596f))
    (pad "5" smd roundrect (at -3.4625 1.27) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SENSE_HIGH") (pinfunction "+") (pintype "input") (tstamp 06f2366d-e2ce-42a9-aa8c-35c7126c4ecc))
    (pad "6" smd roundrect (at -3.4625 2.54) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U2-Pad6)") (pinfunction "-") (pintype "input") (tstamp c89b8f96-266c-4eae-9c58-e3bffa774068))
    (pad "7" smd roundrect (at -3.4625 3.81) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(U2-Pad6)") (pintype "output") (tstamp 7b3da868-deec-40f9-b492-90f9c6130684))
    (pad "8" smd roundrect (at 3.4625 3.81) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U2-Pad9)") (pintype "output") (tstamp 0cd50a40-3019-4666-9ee9-88903b18bccb))
    (pad "9" smd roundrect (at 3.4625 2.54) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U2-Pad9)") (pinfunction "-") (pintype "input") (tstamp b8251e4a-5690-4d85-b658-ebf011b9e806))
    (pad "10" smd roundrect (at 3.4625 1.27) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SENSE_LOW") (pinfunction "+") (pintype "input") (tstamp 0bb29daf-4462-460e-94eb-427040cfc3a2))
    (pad "11" smd roundrect (at 3.4625 0) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in") (tstamp 11053ab2-90b3-4ed4-8cf7-e1fb2f985a8b))
    (pad "12" smd roundrect (at 3.4625 -1.27) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(R10-Pad1)") (pinfunction "+") (pintype "input") (tstamp 238e8734-6852-49da-addd-2d33adaeb5bd))
    (pad "13" smd roundrect (at 3.4625 -2.54) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(R12-Pad2)") (pinfunction "-") (pintype "input") (tstamp 684aa11c-abd6-4faf-aa8b-7a01d9916209))
    (pad "14" smd roundrect (at 3.4625 -3.81) (size 1.975 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R12-Pad1)") (pintype "output") (tstamp c2360e6b-ce35-4f01-a0ce-647566299699))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-14_5.3x10.2mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5_Handsoldering" (layer "F.Cu")
    (tedit 5C9ED275) (tstamp b931c004-c8a7-44ea-b566-da04d3c14ee2)
    (at 134.64 47.72)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/fde06d41-1385-4e9e-8685-30a2a9abf68d")
    (attr smd)
    (fp_text reference "U3" (at 0 -2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b0b2517-d8f1-4fbf-b363-02bffd1f9425)
    )
    (fp_text value "74AHC1GU04" (at 0 2 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 931a4662-758e-4740-82fb-85441aa0a3e1)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
      (tstamp 910738fc-a349-4f37-8d4d-e9cbfb92a52c)
    )
    (fp_line (start -0.7 1.16) (end 0.7 1.16) (layer "F.SilkS") (width 0.12) (tstamp 0e815dda-4411-40dc-97f7-9f0108425575))
    (fp_line (start 0.7 -1.16) (end -1.2 -1.16) (layer "F.SilkS") (width 0.12) (tstamp 6e9ff0eb-b771-4919-b97a-130d58009e2a))
    (fp_line (start -2.4 -1.4) (end -2.4 1.4) (layer "F.CrtYd") (width 0.05) (tstamp 1705a255-1e32-43e5-86c3-8595c54c1346))
    (fp_line (start 2.4 1.4) (end 2.4 -1.4) (layer "F.CrtYd") (width 0.05) (tstamp 4e1c2ec7-0669-4b4d-b78a-5f81536f63b7))
    (fp_line (start -2.4 -1.4) (end 2.4 -1.4) (layer "F.CrtYd") (width 0.05) (tstamp 817fdba7-72a5-40a9-92fc-7556cf5bdc23))
    (fp_line (start -2.4 1.4) (end 2.4 1.4) (layer "F.CrtYd") (width 0.05) (tstamp 97e4af92-bed3-415b-b729-94d9803135a6))
    (fp_line (start 0.675 -1.1) (end 0.675 1.1) (layer "F.Fab") (width 0.1) (tstamp 5e6a694c-6506-47d7-81dd-28e05d1c8345))
    (fp_line (start 0.675 1.1) (end -0.675 1.1) (layer "F.Fab") (width 0.1) (tstamp 87e60dbf-b7a3-4e22-8b26-3ec67ec26fb1))
    (fp_line (start -0.175 -1.1) (end -0.675 -0.6) (layer "F.Fab") (width 0.1) (tstamp ac22bed2-fb05-48e5-8395-d125c53f51c5))
    (fp_line (start 0.675 -1.1) (end -0.175 -1.1) (layer "F.Fab") (width 0.1) (tstamp c66006fa-4b6f-4d53-acd5-09c717ed231b))
    (fp_line (start -0.675 -0.6) (end -0.675 1.1) (layer "F.Fab") (width 0.1) (tstamp ddc0feb1-5ca0-4ba8-a8a9-d1c843dd8a46))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ee39927b-a8be-4807-a1b0-dca9dc072315))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "input") (tstamp d64dd751-0de3-441a-8998-92f27f3966bb))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp a72e2953-0e81-4a58-95d0-62a57c7b5abd))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(R4-Pad2)") (pintype "output") (tstamp 457f6cda-8002-478f-acb9-25cfed27d430))
    (pad "5" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp 42768264-e06d-452d-ae26-7fe95951bd40))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7) (tstamp bd49609d-1fef-4575-9070-13205ced4d1d)
    (at 130.39 57.57)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d22068")
    (attr smd)
    (fp_text reference "D2" (at 0 -2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 15805c4c-6537-4140-8b87-8ff6ac1a0901)
    )
    (fp_text value "DIODESCH" (at 0 2.1) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ee091d6c-1b61-4493-98b3-b0fe3e5c1a98)
    )
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp de869f48-7070-4ed4-8cc8-cf9169b0116f)
    )
    (fp_line (start -2.25 1) (end 1.65 1) (layer "F.SilkS") (width 0.12) (tstamp 15b8bd19-a07e-474b-a062-297cef29b69f))
    (fp_line (start -2.25 -1) (end 1.65 -1) (layer "F.SilkS") (width 0.12) (tstamp b6f0c877-a395-4dd8-8d26-e421251791b9))
    (fp_line (start -2.25 -1) (end -2.25 1) (layer "F.SilkS") (width 0.12) (tstamp d50d052a-8531-489e-8896-b8c664ad26c4))
    (fp_line (start -2.35 -1.15) (end -2.35 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 140a879d-c11e-427b-ab9c-62fdd8a21a25))
    (fp_line (start 2.35 -1.15) (end 2.35 1.15) (layer "F.CrtYd") (width 0.05) (tstamp 6d6fd58e-f30c-446e-8a89-8e324ed7396a))
    (fp_line (start -2.35 -1.15) (end 2.35 -1.15) (layer "F.CrtYd") (width 0.05) (tstamp 82d027f3-df8e-43d0-8280-036b3084c3e1))
    (fp_line (start 2.35 1.15) (end -2.35 1.15) (layer "F.CrtYd") (width 0.05) (tstamp ef128304-dc54-4f5d-95d9-2d3af216bcb2))
    (fp_line (start 1.4 0.9) (end -1.4 0.9) (layer "F.Fab") (width 0.1) (tstamp 0f72957c-fb68-427d-8967-012fd800c604))
    (fp_line (start -0.75 0) (end -0.35 0) (layer "F.Fab") (width 0.1) (tstamp 1007883c-0f39-4bea-9a5a-cee67c90d3ed))
    (fp_line (start -0.35 0) (end -0.35 0.55) (layer "F.Fab") (width 0.1) (tstamp 1875df59-7740-453f-9c5d-80ff945a9832))
    (fp_line (start -0.35 0) (end 0.25 -0.4) (layer "F.Fab") (width 0.1) (tstamp 3bb49748-a9b2-4ace-bacb-a004fe05deff))
    (fp_line (start -1.4 0.9) (end -1.4 -0.9) (layer "F.Fab") (width 0.1) (tstamp 46b9e6e0-6e84-4248-b558-23e679bf6ad5))
    (fp_line (start -0.35 0) (end -0.35 -0.55) (layer "F.Fab") (width 0.1) (tstamp 4e5879ca-19cd-438a-ad6a-ca376b0edb1f))
    (fp_line (start 0.25 0.4) (end -0.35 0) (layer "F.Fab") (width 0.1) (tstamp 8df719fd-3927-481f-8c45-968e501eb641))
    (fp_line (start 0.25 0) (end 0.75 0) (layer "F.Fab") (width 0.1) (tstamp c2c3a1d5-3c24-4025-a84a-447a0c7ec254))
    (fp_line (start 0.25 -0.4) (end 0.25 0.4) (layer "F.Fab") (width 0.1) (tstamp ca92eb1e-990c-45aa-b372-a5ecf86c8ff8))
    (fp_line (start 1.4 -0.9) (end 1.4 0.9) (layer "F.Fab") (width 0.1) (tstamp cba567bb-cbff-407a-82d5-464a9dd431f1))
    (fp_line (start -1.4 -0.9) (end 1.4 -0.9) (layer "F.Fab") (width 0.1) (tstamp e4a931ec-d25c-4f09-b04d-9f03c672523e))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/SENSOR_TRACK") (pinfunction "A") (pintype "passive") (tstamp 81aadf04-f57b-460c-ae86-b0341b76e2bd))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/SENSE_HIGH") (pinfunction "K") (pintype "passive") (tstamp 6d061eef-a275-405f-b42a-570159927e69))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5_Handsoldering" (layer "F.Cu")
    (tedit 5C9ED275) (tstamp d75fc3cf-d9dd-4200-970c-dfd29298bc10)
    (at 119.44 56.53)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/3c08daf0-1b9c-4c60-86a3-9b3525736148")
    (attr smd)
    (fp_text reference "U1" (at 0 -2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 93523b3a-c6fe-4311-9c62-93b14d0d1576)
    )
    (fp_text value "74AHC1GU04" (at 0 2 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f1c30a89-0a0c-4599-8dc3-1b2f4ada09a1)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.075)))
      (tstamp d9fb0e5a-1f0f-49c1-b59f-d6dff5ab795b)
    )
    (fp_line (start -0.7 1.16) (end 0.7 1.16) (layer "F.SilkS") (width 0.12) (tstamp 7ed89c10-68e2-47c6-83d8-ec62cef8d9e5))
    (fp_line (start 0.7 -1.16) (end -1.2 -1.16) (layer "F.SilkS") (width 0.12) (tstamp 9f2048dc-d867-4f7d-ab5e-8ab4f98ac822))
    (fp_line (start 2.4 1.4) (end 2.4 -1.4) (layer "F.CrtYd") (width 0.05) (tstamp a2203736-e818-476d-8b9d-5cba7e8cb72a))
    (fp_line (start -2.4 -1.4) (end 2.4 -1.4) (layer "F.CrtYd") (width 0.05) (tstamp c159dfb4-eb2b-47a8-9b78-a25bde81978d))
    (fp_line (start -2.4 -1.4) (end -2.4 1.4) (layer "F.CrtYd") (width 0.05) (tstamp c3f4efa7-2e25-4b4d-8de2-3b30411de9d0))
    (fp_line (start -2.4 1.4) (end 2.4 1.4) (layer "F.CrtYd") (width 0.05) (tstamp f1815d93-506f-4819-9eed-50dfdf489e72))
    (fp_line (start -0.675 -0.6) (end -0.675 1.1) (layer "F.Fab") (width 0.1) (tstamp 4b1cb7b6-0dcd-4d19-8ed3-6a520b9beca9))
    (fp_line (start 0.675 1.1) (end -0.675 1.1) (layer "F.Fab") (width 0.1) (tstamp 85791d1a-588b-4c0d-9ce4-7db6804f2742))
    (fp_line (start -0.175 -1.1) (end -0.675 -0.6) (layer "F.Fab") (width 0.1) (tstamp aa5a1624-5081-4612-bf51-1c8e679e5568))
    (fp_line (start 0.675 -1.1) (end 0.675 1.1) (layer "F.Fab") (width 0.1) (tstamp bf2dcfcc-2a13-4316-87e4-4edd4c6c3601))
    (fp_line (start 0.675 -1.1) (end -0.175 -1.1) (layer "F.Fab") (width 0.1) (tstamp d1cf0ba5-2abf-4bee-8620-eba60dcc21ee))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 48763695-bd2a-4786-a7d0-b3efc65264f2))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pintype "input") (tstamp f291d01c-37e6-47b8-9c3d-d0b5e8acdae3))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 77b270fc-bb9a-4675-b5b2-2ff60ff44dc7))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "output") (tstamp 39c934c5-cc83-49c7-936c-26b32b06245c))
    (pad "5" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in") (tstamp c12cfbc0-5675-48fe-b5c7-5007662b474f))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp dc39350d-e454-4ee2-b02e-b27eec92b90e)
    (at 148.59 52.07)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d21881")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a85f4758-4da0-4632-8404-56a075d81149)
    )
    (fp_text value "18p" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 720dd9ad-100a-48de-ac7a-9d4a3c89247d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 4b54f45c-af9c-4625-b6a7-c75b91fa8688)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 4eed3a96-ad41-4273-93f7-a763863270ed))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp b354e803-efce-46e3-ba61-e6e311ac19d1))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3c12bd17-6c2b-4b5b-bb83-7102a2728f28))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8e73152a-416d-447c-9c0f-e6fea5aa2b74))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp dd8dd57b-ef75-40b6-9a3f-42a9d3ad79ba))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp f779e539-6192-4070-95a6-f5aa338d4d35))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 0e982402-64e6-4ed1-89d7-2c3f1187d7dc))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 52f6690d-fc3f-40c4-86e4-f0d7223eccdd))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 72570411-d58c-40ba-baf8-4a1239e1199f))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp bec8303c-8931-4b5c-9f24-8288bfc49d8f))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pintype "passive") (tstamp ef1905c4-1850-43f2-abab-1d753c7c38d5))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 73a5e5b5-f85a-4b37-bd06-f28de87c0dea))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp e00d634c-76e3-451e-8bc7-a12ae9a630f3)
    (at 127.94 65.05)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d2b12f")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5836f434-b0ba-464c-90c2-bc782fc481fb)
    )
    (fp_text value "10k 0.1%" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ac405e26-c6ec-4174-9c59-12337f43f64f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 5c5b8174-fc78-425a-9586-50a09e472997)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 1f8a5d9f-598a-4343-8f4f-2c6c3324825d))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 975af3dc-078b-49f0-b909-f94732d3aa0a))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1b99d0f1-86e7-4273-9bea-3e494df4ee79))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5a5fadfd-ac4a-443b-9726-9890d0cb04a2))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 85447e9f-dcf8-4e4c-ba9c-14fd243ebca5))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp fde76fd3-edc8-4aad-b56f-8099e7cc03c0))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 0c856df1-863b-4822-a434-34e727304c63))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d0d83370-ba21-4146-ba58-d224c706153d))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp eff1fad5-ba2d-4f08-9c70-94e39efb75a7))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp fb6ec269-5153-4fb3-9107-acbfbebe3813))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(R12-Pad2)") (pintype "passive") (tstamp 21d9e9e3-b90b-44d0-89da-230943e77252))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(U2-Pad9)") (pintype "passive") (tstamp 0cb199a5-6f88-45b6-b6eb-aaa22927fadf))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Crystal:Crystal_SMD_HC49-SD" (layer "F.Cu")
    (tedit 5A1AD52C) (tstamp e5326695-6ec9-4736-a7ac-3e84923f6bfd)
    (at 105.41 63.94 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d213ea")
    (attr smd)
    (fp_text reference "X1" (at 0 -3.55 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d730515-ef52-4e1c-9aab-e1ac25df49bb)
    )
    (fp_text value "16MHz" (at 0 3.55 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 876ced2d-e822-4163-bf95-f1aa79fb9582)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c21422c-8777-4ee6-8901-50bcfd7479cf)
    )
    (fp_line (start -6.7 -2.55) (end -6.7 2.55) (layer "F.SilkS") (width 0.12) (tstamp 334c063e-73c0-4f31-98ba-dabfe56ba7bf))
    (fp_line (start -6.7 2.55) (end 5.9 2.55) (layer "F.SilkS") (width 0.12) (tstamp 3b37349f-6029-44c4-89f9-043f8f755093))
    (fp_line (start 5.9 -2.55) (end -6.7 -2.55) (layer "F.SilkS") (width 0.12) (tstamp e276325f-35bb-48d4-ac6f-e371f594e7ae))
    (fp_line (start -6.8 2.6) (end 6.8 2.6) (layer "F.CrtYd") (width 0.05) (tstamp 003fb8f6-ff99-4211-9ed8-0b1118446f7b))
    (fp_line (start 6.8 -2.6) (end -6.8 -2.6) (layer "F.CrtYd") (width 0.05) (tstamp 7c934d00-6661-4590-b06a-3a688254b4d1))
    (fp_line (start 6.8 2.6) (end 6.8 -2.6) (layer "F.CrtYd") (width 0.05) (tstamp 81236026-b024-4445-9ef8-e0adbab4a389))
    (fp_line (start -6.8 -2.6) (end -6.8 2.6) (layer "F.CrtYd") (width 0.05) (tstamp db191379-29dc-4b70-9d60-520ffc87388e))
    (fp_line (start -3.015 -2.115) (end 3.015 -2.115) (layer "F.Fab") (width 0.1) (tstamp 048274d2-43d9-4a31-9de3-f17a70bc20b3))
    (fp_line (start -5.7 -2.35) (end -5.7 2.35) (layer "F.Fab") (width 0.1) (tstamp 0548f591-fccb-4fe3-a7d6-5b941b1bc25c))
    (fp_line (start 5.7 2.35) (end 5.7 -2.35) (layer "F.Fab") (width 0.1) (tstamp b79096f8-00ec-48ac-b288-7d100d7f364f))
    (fp_line (start -3.015 2.115) (end 3.015 2.115) (layer "F.Fab") (width 0.1) (tstamp bd3f4035-7a71-44e6-be72-acfd894277ed))
    (fp_line (start 5.7 -2.35) (end -5.7 -2.35) (layer "F.Fab") (width 0.1) (tstamp f60f7c44-fc74-4427-819e-861c07cc9b70))
    (fp_line (start -5.7 2.35) (end 5.7 2.35) (layer "F.Fab") (width 0.1) (tstamp ff15b0df-447e-4044-873b-6acb27718e42))
    (fp_arc (start -3.015 2.115) (mid -5.13 0) (end -3.015 -2.115) (layer "F.Fab") (width 0.1) (tstamp 6ff27160-cc9e-49fc-b084-3976471987da))
    (fp_arc (start 3.015 -2.115) (mid 5.13 0) (end 3.015 2.115) (layer "F.Fab") (width 0.1) (tstamp 96818ffa-d780-4f27-8821-5dc12d4dcca3))
    (pad "1" smd rect (at -4.25 0 90) (size 4.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 2b01bd82-b457-40a9-9fa4-a13a052af50f))
    (pad "2" smd rect (at 4.25 0 90) (size 4.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "2") (pintype "passive") (tstamp 6c268b15-3021-44c1-8fc0-fc861ecbaa66))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp f16202a3-b8df-476e-87ad-ace6a314a142)
    (at 132.29 63.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-000054d221c8")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78c20f43-57fb-42f8-9270-9fbf4c25b948)
    )
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b8c31afb-025f-4824-87ac-e1554ee01ad9)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 5df1c4a3-09a2-457f-93e6-ba9584b14ce7)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 9896821e-4711-4fb7-a760-8028f7e0d0d7))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp e0081891-c59d-4c8c-8abd-e56fe809d635))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3d3c8a1c-5ae0-40e7-bc29-cae9e1824608))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 73d9dec1-ee54-437a-a2d0-c4b924c3e24b))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 78ca71d4-75e8-43ac-8a4b-cbeabbff4669))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e4a05207-4a17-4e19-85fc-121d9e36e8e7))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 0253f5a1-e403-48c1-8081-203a52701a12))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 337f17ac-bb51-4977-82e8-56445ea266d7))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 4eed432c-c262-4824-acc6-d6c57f7cecb6))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 58d0bd8d-4aa1-4a75-b403-14ce2e24badb))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 4b526753-d1c8-45f2-a3ae-e7cf9305a9cd))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SENSE_HIGH") (pintype "passive") (tstamp 813bdc0d-50cc-4a35-996b-86881ea4fe53))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp fda9a66d-d84e-4cf9-876c-042d1874d1a1)
    (at 145.49 47.05)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/media/fisch/HDD/Projects/hydroponik/soil-moisture-sensor-analog/analog-moist-sensor.sch")
    (property "Sheetname" "")
    (path "/00000000-0000-0000-0000-0000551426a3")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3506bcc8-f35f-4fe3-b8d6-9cfd512d8987)
    )
    (fp_text value "330" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 182eb4d0-bde4-4b8c-8191-0dbbca9d70b7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 0ee7f924-ad4b-44f5-9281-e917c0f3f8d4)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 56dc8aab-9328-4420-a00b-bc84c9d1808f))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp ce9406d1-e10f-4802-aaad-b099e837cd34))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 6839f1d1-7a8e-4692-8821-b7ee6f3251b6))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9e0659a3-f7b3-43ca-97a7-f608555063f9))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp a18748b0-325f-4c54-a1d3-84a59df9036f))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp fa903eb6-d45b-4a08-9207-3f72c713d66c))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 55e99fec-51a8-4dc1-96eb-82183fdd9527))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7ac97a26-5a4c-4116-a60d-925301a5f5b9))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 9870c00e-e3c4-448c-8271-726360b1d2f9))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp df1bb6f2-78c4-4967-a512-66af47901947))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/OUT") (pintype "passive") (tstamp ca3edca0-e658-4092-b7ec-f64e9a3f956c))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R13-Pad2)") (pintype "passive") (tstamp 049b9c98-d699-4554-be3b-ab5531113a6a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 99.032 28.225286) (end 114.272 28.225286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30220))
  (gr_line (start 99.032 30.535286) (end 99.032 28.225286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30221))
  (gr_line (start 114.272 30.535286) (end 114.272 28.225286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30222))
  (gr_line (start 114.272 30.535286) (end 114.272 33.075286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30223))
  (gr_line (start 99.032 33.075286) (end 99.032 30.535286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30224))
  (gr_line (start 114.272 71.175286) (end 114.272 132.135286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30225))
  (gr_line (start 99.032 132.135286) (end 99.032 71.175286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30227))
  (gr_line (start 106.652 142.422286) (end 114.272 132.135286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30228))
  (gr_line (start 99.032 132.135286) (end 106.652 142.422286) (layer "Edge.Cuts") (width 0.1) (tstamp 00000000-0000-0000-0000-000054e30229))
  (dimension (type aligned) (layer "Cmts.User") (tstamp 00000000-0000-0000-0000-000054e302c4)
    (pts (xy 99.159 36.203286) (xy 114.145 36.203286))
    (height -14.05)
    (gr_text "14.9860 mm" (at 106.652 20.353286) (layer "Cmts.User") (tstamp 00000000-0000-0000-0000-000054e302c4)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User") (tstamp 00000000-0000-0000-0000-000054e302c6)
    (pts (xy 99 142.5) (xy 98.806 28.448))
    (height -8.607523)
    (gr_text "114.0522 mm" (at 92.095486 85.485579 -89.9025412) (layer "Cmts.User") (tstamp 00000000-0000-0000-0000-000054e302c6)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User") (tstamp cc3ea537-bd02-4538-9f9a-20af938ab55e)
    (pts (xy 106.652 81.081286) (xy 106.652 133.405286))
    (height -16.256)
    (gr_text "52.3240 mm" (at 121.108 107.243286 90) (layer "Cmts.User") (tstamp cc3ea537-bd02-4538-9f9a-20af938ab55e)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )

  (segment (start 106.652 86.967) (end 106.68 86.995) (width 0.254) (layer "F.Cu") (net 5) (tstamp 17b605e3-f755-4a96-9369-1c5387732102))
  (segment (start 106.68 131.445) (end 106.68 86.995) (width 5) (layer "F.Cu") (net 5) (tstamp 90b37e3d-a849-46a0-aa52-4a4da9edd3b3))
  (segment (start 106.652 85.145286) (end 106.652 86.967) (width 0.254) (layer "F.Cu") (net 5) (tstamp a3d3baf1-209a-4861-b9f8-c5b3c5cfb657))
  (segment (start 106.652 85.145286) (end 106.652 72.656723) (width 0.508) (layer "F.Cu") (net 5) (tstamp a5c429cd-b864-4cb2-a18c-252c9e93d6b9))

  (zone (net 2) (net_name "GND") (layer "F.Cu") (tstamp 00000000-0000-0000-0000-000054e3055b) (hatch edge 0.508)
    (connect_pads (clearance 0.2286))
    (min_thickness 0.254)
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.048 28.448)
        (xy 113.256 28.448)
        (xy 113.256 82.804)
        (xy 113.256 83.058)
        (xy 113.256 133.604)
        (xy 106.652 142.24)
        (xy 100.242236 133.858)
        (xy 100.048 133.858)
        (xy 100.048 133.604)
        (xy 100.048 83.058)
      )
    )
    (polygon
      (pts
        (xy 102.632 84.108)
        (xy 102.632 132.108)
        (xy 104.632 135.108)
        (xy 108.632 135.108)
        (xy 110.632 132.108)
        (xy 110.632 84.108)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (tstamp 00000000-0000-0000-0000-000054e30756) (hatch edge 0.508)
    (connect_pads (clearance 0.2286))
    (min_thickness 0.254)
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.048 28.448)
        (xy 113.256 28.448)
        (xy 113.284 84.780714)
        (xy 100.076 84.780714)
      )
    )
  )
)
