(export (version D)
  (design
    (source /media/fisch/HDD/Projects/audiomixer/schematic/mixerin_output/mixerin_output.sch)
    (date "Fr 09 Aug 2019 15:31:02 CEST")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source mixerin_output.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J3)
      (value Conn_02x18_Row_Letter_First)
      (footprint footprints:PCIexpress_1x_letters)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x18_Row_Letter_Last) (description "Generic connector, double row, 02x18, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C5482AB))
    (comp (ref U1)
      (value LM4562)
      (footprint Package_DIP:DIP-8_W7.62mm)
      (libsource (lib Device) (part Opamp_Dual_Generic) (description "Dual operational amplifier"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CA7D))
    (comp (ref RA2)
      (value 10k|0|open)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CA8C))
    (comp (ref RA1)
      (value 10k|10k|0)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CA95))
    (comp (ref RA3)
      (value 10k|1k|10k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAA4))
    (comp (ref RA5)
      (value 10k|open|open)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAAC))
    (comp (ref RA4)
      (value 10|0|open)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAB9))
    (comp (ref JA2)
      (value Jumper)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CACC))
    (comp (ref RB2)
      (value 10k|0|open)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAD8))
    (comp (ref RB3)
      (value 10k|1k|10k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAE4))
    (comp (ref RB5)
      (value 10k|open|open)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAEC))
    (comp (ref RB4)
      (value 10|0|open)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CAF8))
    (comp (ref JB1)
      (value Jumper)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CB0B))
    (comp (ref RB1)
      (value 10k|10k|0)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CB19))
    (comp (ref C1)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CB2B))
    (comp (ref C2)
      (value 100n)
      (footprint Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C54CB3A))
    (comp (ref RA6)
      (value 0|0|220)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA39C35))
    (comp (ref RB6)
      (value 0|0|220)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (fields
        (field (name Notes) Metallfilm))
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA3D551))
    (comp (ref ClpA1)
      (value 330p)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA42A5F))
    (comp (ref ClpB1)
      (value 330p)
      (footprint Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CA46ED4)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x18_Row_Letter_Last)
      (description "Generic connector, double row, 02x18, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x18_Row_Letter_Last))
      (pins
        (pin (num 1a) (name Pin_1a) (type passive))
        (pin (num 1b) (name Pin_1b) (type passive))
        (pin (num 2a) (name Pin_2a) (type passive))
        (pin (num 2b) (name Pin_2b) (type passive))
        (pin (num 3a) (name Pin_3a) (type passive))
        (pin (num 3b) (name Pin_3b) (type passive))
        (pin (num 4a) (name Pin_4a) (type passive))
        (pin (num 4b) (name Pin_4b) (type passive))
        (pin (num 5a) (name Pin_5a) (type passive))
        (pin (num 5b) (name Pin_5b) (type passive))
        (pin (num 6a) (name Pin_6a) (type passive))
        (pin (num 6b) (name Pin_6b) (type passive))
        (pin (num 7a) (name Pin_7a) (type passive))
        (pin (num 7b) (name Pin_7b) (type passive))
        (pin (num 8a) (name Pin_8a) (type passive))
        (pin (num 8b) (name Pin_8b) (type passive))
        (pin (num 9a) (name Pin_9a) (type passive))
        (pin (num 9b) (name Pin_9b) (type passive))
        (pin (num 10a) (name Pin_10a) (type passive))
        (pin (num 10b) (name Pin_10b) (type passive))
        (pin (num 11a) (name Pin_11a) (type passive))
        (pin (num 11b) (name Pin_11b) (type passive))
        (pin (num 12a) (name Pin_12a) (type passive))
        (pin (num 12b) (name Pin_12b) (type passive))
        (pin (num 13a) (name Pin_13a) (type passive))
        (pin (num 13b) (name Pin_13b) (type passive))
        (pin (num 14a) (name Pin_14a) (type passive))
        (pin (num 14b) (name Pin_14b) (type passive))
        (pin (num 15a) (name Pin_15a) (type passive))
        (pin (num 15b) (name Pin_15b) (type passive))
        (pin (num 16a) (name Pin_16a) (type passive))
        (pin (num 16b) (name Pin_16b) (type passive))
        (pin (num 17a) (name Pin_17a) (type passive))
        (pin (num 17b) (name Pin_17b) (type passive))
        (pin (num 18a) (name Pin_18a) (type passive))
        (pin (num 18b) (name Pin_18b) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Opamp_Dual_Generic)
      (description "Dual operational amplifier")
      (docs ~)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*)
        (fp DIP*W7.62mm*)
        (fp MSOP*3x3mm*P0.65mm*)
        (fp SSOP*2.95x2.8mm*P0.65mm*)
        (fp TSSOP*3x3mm*P0.65mm*)
        (fp VSSOP*P0.5mm*)
        (fp TO?99*))
      (fields
        (field (name Reference) U)
        (field (name Value) Opamp_Dual_Generic))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name V+) (type power_in))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib)))
  (nets
    (net (code 1) (name -15V)
      (node (ref J3) (pin 3b))
      (node (ref J3) (pin 1b))
      (node (ref C2) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref J3) (pin 2b))
      (node (ref J3) (pin 3a))
      (node (ref J3) (pin 2a))
      (node (ref J3) (pin 1a)))
    (net (code 2) (name +15V)
      (node (ref J3) (pin 9b))
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref J3) (pin 8b))
      (node (ref J3) (pin 7a))
      (node (ref J3) (pin 7b))
      (node (ref J3) (pin 8a))
      (node (ref J3) (pin 9a)))
    (net (code 3) (name inA-)
      (node (ref J3) (pin 12a))
      (node (ref RA2) (pin 1)))
    (net (code 4) (name GNDA)
      (node (ref C1) (pin 2))
      (node (ref J3) (pin 6b))
      (node (ref RB4) (pin 2))
      (node (ref RB5) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref J3) (pin 18b))
      (node (ref J3) (pin 4a))
      (node (ref J3) (pin 4b))
      (node (ref J3) (pin 5a))
      (node (ref J3) (pin 5b))
      (node (ref RA4) (pin 2))
      (node (ref J3) (pin 10a))
      (node (ref J3) (pin 10b))
      (node (ref J3) (pin 15b))
      (node (ref J3) (pin 11b))
      (node (ref J3) (pin 12b))
      (node (ref J3) (pin 13a))
      (node (ref J3) (pin 15a))
      (node (ref J3) (pin 11a))
      (node (ref J3) (pin 6a))
      (node (ref RA5) (pin 2))
      (node (ref J3) (pin 17a)))
    (net (code 5) (name "Net-(ClpB1-Pad1)")
      (node (ref U1) (pin 7))
      (node (ref ClpB1) (pin 1))
      (node (ref RB1) (pin 2))
      (node (ref RB6) (pin 1)))
    (net (code 6) (name "Net-(RB3-Pad2)")
      (node (ref U1) (pin 5))
      (node (ref RB3) (pin 2))
      (node (ref RB5) (pin 1)))
    (net (code 7) (name inB+)
      (node (ref J3) (pin 18a))
      (node (ref RB3) (pin 1))
      (node (ref JB1) (pin 1)))
    (net (code 8) (name "Net-(JB1-Pad2)")
      (node (ref RB4) (pin 1))
      (node (ref JB1) (pin 2)))
    (net (code 9) (name "Net-(ClpA1-Pad1)")
      (node (ref RA1) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref ClpA1) (pin 1))
      (node (ref RA6) (pin 1)))
    (net (code 10) (name "Net-(ClpB1-Pad2)")
      (node (ref ClpB1) (pin 2))
      (node (ref U1) (pin 6))
      (node (ref RB2) (pin 2))
      (node (ref RB1) (pin 1)))
    (net (code 11) (name outA)
      (node (ref RA6) (pin 2))
      (node (ref J3) (pin 14b))
      (node (ref J3) (pin 13b)))
    (net (code 12) (name outB)
      (node (ref J3) (pin 17b))
      (node (ref J3) (pin 16b))
      (node (ref RB6) (pin 2)))
    (net (code 13) (name inB-)
      (node (ref RB2) (pin 1))
      (node (ref J3) (pin 16a)))
    (net (code 14) (name inA+)
      (node (ref JA2) (pin 1))
      (node (ref J3) (pin 14a))
      (node (ref RA3) (pin 1)))
    (net (code 15) (name "Net-(ClpA1-Pad2)")
      (node (ref ClpA1) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref RA2) (pin 2))
      (node (ref RA1) (pin 1)))
    (net (code 16) (name "Net-(RA3-Pad2)")
      (node (ref RA5) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref RA3) (pin 2)))
    (net (code 17) (name "Net-(JA2-Pad2)")
      (node (ref JA2) (pin 2))
      (node (ref RA4) (pin 1)))))