(export (version D)
  (design
    (source /media/fisch/HDD/Projects/hoverbrett/powerlatch/powerlatch.sch)
    (date "Sa 07 Dez 2019 13:27:22 CET")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu16.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source powerlatch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref Q2)
      (value TIP127)
      (footprint Package_TO_SOT_THT:TO-220-3_Vertical)
      (datasheet http://www.fairchildsemi.com/ds/TI/TIP125.pdf)
      (libsource (lib Transistor_BJT) (part TIP127) (description "5A Ic, 100V Vce, Silicon Darlington Power PNP Transistor, TO-220"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAE833))
    (comp (ref Q1)
      (value 2N5551)
      (footprint Package_TO_SOT_THT:TO-92L_Inline_Wide)
      (datasheet ~)
      (libsource (lib Device) (part Q_NPN_EBC) (description "NPN transistor, emitter/base/collector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAEC02))
    (comp (ref R5)
      (value 51k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAECF1))
    (comp (ref R6)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAEE16))
    (comp (ref R7)
      (value 51k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAF12D))
    (comp (ref R3)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAF5A5))
    (comp (ref D1)
      (value 1N4007)
      (footprint Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal)
      (datasheet http://www.vishay.com/docs/88503/1n4001.pdf)
      (libsource (lib Diode) (part 1N4007) (description "1000V 1A General Purpose Rectifier Diode, DO-41"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAF799))
    (comp (ref R4)
      (value 2k2)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAF884))
    (comp (ref R2)
      (value 2k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEAFAB1))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB1238))
    (comp (ref R1)
      (value 30k)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB1A23))
    (comp (ref J2)
      (value switched+)
      (footprint TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB2370))
    (comp (ref J3)
      (value switched-)
      (footprint TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB242C))
    (comp (ref J1)
      (value enable)
      (footprint TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB2BD6))
    (comp (ref J4)
      (value Bat+)
      (footprint TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB3053))
    (comp (ref J5)
      (value Bat-)
      (footprint TestPoint:TestPoint_THTPad_1.5x1.5mm_Drill0.7mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DEB30F7)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x01)
      (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib Device) (part Q_NPN_EBC)
      (description "NPN transistor, emitter/base/collector")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_EBC))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Diode) (part 1N4001)
      (aliases
        (alias 1N4002)
        (alias 1N4003)
        (alias 1N4004)
        (alias 1N4005)
        (alias 1N4006)
        (alias 1N4007)
        (alias BA157)
        (alias BA158)
        (alias BA159))
      (description "50V 1A General Purpose Rectifier Diode, DO-41")
      (docs http://www.vishay.com/docs/88503/1n4001.pdf)
      (footprints
        (fp D*DO?41*))
      (fields
        (field (name Reference) D)
        (field (name Value) 1N4001)
        (field (name Footprint) Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Transistor_BJT) (part TIP125)
      (aliases
        (alias TIP126)
        (alias TIP127))
      (description "5A Ic, 60V Vce, Silicon Darlington Power PNP Transistor, TO-220")
      (docs http://www.fairchildsemi.com/ds/TI/TIP125.pdf)
      (footprints
        (fp TO?220*))
      (fields
        (field (name Reference) Q)
        (field (name Value) TIP125)
        (field (name Footprint) Package_TO_SOT_THT:TO-220-3_Vertical))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name C) (type passive))
        (pin (num 3) (name E) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Diode)
      (uri /usr/share/kicad/library/Diode.lib))
    (library (logical Switch)
      (uri /usr/share/kicad/library/Switch.lib))
    (library (logical Transistor_BJT)
      (uri /usr/share/kicad/library/Transistor_BJT.lib)))
  (nets
    (net (code 1) (name "Net-(D1-Pad2)")
      (node (ref SW1) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 2) (name GND)
      (node (ref J3) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref J5) (pin 1)))
    (net (code 3) (name "Net-(R1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref SW1) (pin 2)))
    (net (code 4) (name "Net-(J1-Pad1)")
      (node (ref R4) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 5) (name "Net-(D1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 6) (name +BATT)
      (node (ref R1) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref R7) (pin 1))
      (node (ref J4) (pin 1)))
    (net (code 7) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1))
      (node (ref Q2) (pin 2)))
    (net (code 8) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 9) (name "Net-(Q1-Pad2)")
      (node (ref R4) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref R5) (pin 1)))
    (net (code 10) (name "Net-(Q1-Pad3)")
      (node (ref Q1) (pin 3))
      (node (ref R6) (pin 2)))))